{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":3,"rows_kept":28,"merged":[[0,0,0,2],[2,1,5,1],[6,1,8,1],[9,1,12,1],[13,1,14,1],[27,0,27,2]],"flags":["formulas_cached_only"]}
["附着式升降脚手架委托检验检测内容"]
["序号","检验检测项 目","具体内容需要符合规范要求"]
[1,"现场资料","安装后的自检记录应完整齐全"]
[2,null,"出厂检验合格证符合要求"]
[3,null,"论证通过的专项施工方案"]
[4,null,"附着式升降脚手架机位布置图"]
[5,"主框架和水平桁架","各节点应焊接或螺栓连接"]
[6,null,"桁架上、下弦应采用整根通长杆件，或设置刚性接头；腹杆上、下弦连接应采用焊接或螺栓连接"]
[7,null,"桁架各杆件的轴线应相交于节点上，并宜用节点板构造连接，节点板的厚度不得小于6mm"]
[8,"架体构造尺寸","架体高度≤5倍楼层高"]
[9,null,"架体宽度≤1.2 m"]
[10,null,"直线布置的架体支承跨度≤7 m"]
[11,null,"架体全高与支承跨度的乘积≤110 ㎡"]
[12,"升降装置","应在每个竖向主框架处设置升降设备"]
[13,null,"应采用电动葫芦或电动液压设备"]
[14,"防坠落","应设置在竖向主框架处并附着在建筑结构上"]
[15,"装置","每一升降点不得少于一个防坠落装置"]
[16,null,"防坠落装置应采用机械式的全自动装置"]
[17,null,"防坠落装置应具有防尘、防污染的措施"]
[18,null,"防坠落装置与升降设备应分别独立固定在建筑结构上"]
[19,null,"钢吊杆式防坠落装置，不应小于ф25mm"]
[20,"防倾覆","防倾覆装置中应包括导轨和两个以上与导轨连接的可滑动的导向件"]
[21,"装置","在防倾导向件的范围内应设置防倾覆导轨,且应与竖向主框架可靠连接"]
[22,null,"最上和最下两个导向件之间的最小间距不得小于2.8m或架体高度的1/4"]
[23,null,"防倾覆装置中的导向件通过螺栓连接固定在附墙支座上"]
[24,null,"应采用螺栓与附墙支座连接，其装置与导轨之间的间隙应小于5mm"]
[25,"同步控制系统","连续式水平支承桁架，应采用限制荷载自控系统"]
["备注:根据新的附着式升降脚手架型号，适当增加相应的检验检测内容"]

{"sheet":"Sheet2","index":1,"n_rows":27,"n_cols":3,"rows_kept":27,"merged":[[1,1,4,1],[5,1,7,1],[8,1,11,1],[12,1,13,1],[26,0,26,2]],"flags":["formulas_cached_only"]}
["序号","检验检测项 目","具体内容需要符合规范要求"]
[1,"现场资料","安装后的自检记录应完整齐全"]
[2,null,"出厂检验合格证符合要求"]
[3,null,"论证通过的专项施工方案"]
[4,null,"附着式升降脚手架机位布置图"]
[5,"主框架和水平桁架","各节点应焊接或螺栓连接"]
[6,null,"桁架上、下弦应采用整根通长杆件，或设置刚性接头；腹杆上、下弦连接应采用焊接或螺栓连接"]
[7,null,"桁架各杆件的轴线应相交于节点上，并宜用节点板构造连接，节点板的厚度不得小于6mm"]
[8,"架体构造尺寸","架体高度≤5倍楼层高"]
[9,null,"架体宽度≤1.2 m"]
[10,null,"直线布置的架体支承跨度≤7 m"]
[11,null,"架体全高与支承跨度的乘积≤110 ㎡"]
[12,"升降装置","应在每个竖向主框架处设置升降设备"]
[13,null,"应采用电动葫芦或电动液压设备"]
[14,"防坠落","应设置在竖向主框架处并附着在建筑结构上"]
[15,"装置","每一升降点不得少于一个防坠落装置"]
[16,null,"防坠落装置应采用机械式的全自动装置"]
[17,null,"防坠落装置应具有防尘、防污染的措施"]
[18,null,"防坠落装置与升降设备应分别独立固定在建筑结构上"]
[19,null,"钢吊杆式防坠落装置，不应小于ф25mm"]
[20,"防倾覆","防倾覆装置中应包括导轨和两个以上与导轨连接的可滑动的导向件"]
[21,"装置","在防倾导向件的范围内应设置防倾覆导轨,且应与竖向主框架可靠连接"]
[22,null,"最上和最下两个导向件之间的最小间距不得小于2.8m或架体高度的1/4"]
[23,null,"防倾覆装置中的导向件通过螺栓连接固定在附墙支座上"]
[24,null,"应采用螺栓与附墙支座连接，其装置与导轨之间的间隙应小于5mm"]
[25,"同步控制系统","连续式水平支承桁架，应采用限制荷载自控系统"]
["备注:根据新的附着式升降脚手架型号，适当增加相应的检验检测内容"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}