{"text_format":"3","workbook":"xls","n_sheets":16,"sheets":["Sheet1","Sheet2","Sheet3","Sheet4","Sheet5","Sheet6","Sheet7","Sheet8","Sheet9","Sheet10","Sheet11","Sheet12","Sheet13","Sheet14","Sheet15","Sheet16"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"flags":["formulas_cached_only"]}
["选用的主要施工机械一览表"]
[]
["序号","机具名称","规格","数量","功率(KW)","备注"]
[1,"滑行式柴油发电机","SC120-BG","1台","120/台"]
[2,"回转钻机机组","GPS-15","3套","50/套"]
[3,"深层搅拌机机组","SJB-1","2套","75/套"]
[4,"抓斗吊","自制","2台","4/台"]
[5,"轻型井点系统","V5型","2套","11.5/套"]
[6,"液压反铲挖土机","1.2M3","2台","自备"]
[7,"履带吊",null,"2台","自备"]
[8,"自卸汽车","15吨","10台","自备"]
[9,"塔吊","JL160","1台","94/台"]
[10,"砂浆搅拌机","250型","1台"]
[11,"砼地泵","BSA1405/06","1台","75/台"]
[12,"插入式振捣棒","HZ650","10只","2/台"]
[13,"平板式振捣器",null,"1台"]
[14,"钢筋闪光对焊机",null,"2台"]
[15,"交流电焊机","BX3-300","2台","20/台"]
[16,"钢筋切断机","QJ40-1","1台","5.5/台"]
[17,"钢筋调直机","4-14mm","1台","9.5/台"]
[18,"钢筋弯曲机","WL40-1","1台","3/台"]
[19,"电锯","MG235","2台","4/台"]
[20,"压刨","MB-106","2台","5.5/台"]
[21,"平刨","MB-503A","2台","3/台"]
[22,"激光垂准仪",null,"1台"]
[23,"经纬仪","JZ-JD2","1台"]
[24,"水准仪",null,"1台"]
[25,"消防泵",null,"5台"]
[26,"潜水泵","8NQ50-18","8台","2.5/台"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet4","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet5","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet6","index":5,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet7","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet8","index":7,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet9","index":8,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet10","index":9,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet11","index":10,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet12","index":11,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet13","index":12,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet14","index":13,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet15","index":14,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet16","index":15,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}