{"text_format":"3","workbook":"xls","n_sheets":62,"sheets":["母表(1)","母表(2)","(一)煤炭（1）","(一)煤炭（2）","（二）化工石化医药（1） ","（二）化工石化医药（2） ","（三）石油天然气（1）","（三）石油天然气（2）","（四）电力（1）","（四）电力（2）","（五）冶金（1）","（五）冶金（2）","（六）军工（1）","（六）军工（2）","（七）机械（1）","（七）机械（2）","（八）商物粮（1）","（八）商物粮（2）","（九）核工业（1）","（九）核工业（2）","（十）电子通信广电（1）","（十）电子通信广电（2）","（十一）轻纺（1）","（十一）轻纺（2）","（十二）建材（1）","（十二）建材（2）","（十三）铁道（1）","（十三）铁道（2）","（十四）公路（1）","（十四）公路（2）","（十五）水运（1）","（十五）水运（2）","（十六）民航（1）","（十六）民航（2）","（十七）市政（1）","（十七）市政（2）","（十八）海洋（1）","（十八）海洋（2）","（十九）水利（1）","（十九）水利（2）","（二十）农林（1）","（二十）农林（2）","（二十一）建筑（1）A","（二十一）建筑（1）B","（二十一）建筑（2）A","（二十一）建筑（2）B","（1）建筑装饰A","（1）建筑装饰B","（2）建筑智能化A","（2）建筑智能化B","（3）建筑幕墙A","（3）建筑幕墙B","（4）钢结构A","（4）钢结构B","（5）园林景观A","（5）园林景观B","（6）消防设施A","（6）消防设施B","（7）环境A","（7）环境B","（8）防腐A","（8）防腐B"],"not_rendered":{"external_links":1,"defined_names":25},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"母表(1)","index":0,"n_rows":10,"n_cols":27,"rows_kept":10,"merged":[[0,0,1,2],[0,25,1,25],[0,26,1,26],[2,0,3,0],[2,1,2,2],[3,1,3,2],[4,0,9,0]],"flags":["formulas_cached_only"]}
[{"$nulls":3},"采矿","露采","选煤","矿山机电","机械","电力","电气","建筑","结构","给排水","暖通空调","环保","总图","运输","技术经济",{"$nulls":7},"总计","备   注"]
[{"$nulls":3},"采矿/矿物 采矿","采矿/矿物 采矿","采矿/矿物 采矿",null,"机械",null,"电气  供配电","二级及以上建筑师","一级结构工程师","公用设备","公用设备","环保",null,null,"造价"]
["行业\n资质",{"$nulls":24},0]
[{"$nulls":25},0]
["专业\n资质",{"$nulls":24},0]
[{"$nulls":25},0]
[{"$nulls":25},0]
[{"$nulls":25},0]
[{"$nulls":25},0]
[{"$nulls":25},0]

{"sheet":"母表(2)","index":1,"n_rows":1,"n_cols":7,"rows_kept":1,"flags":["formulas_cached_only"]}
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]

{"sheet":"(一)煤炭（1）","index":2,"n_rows":14,"n_cols":22,"rows_kept":14,"merged":[[0,0,0,21],[1,0,2,2],[1,20,2,20],[1,21,2,21],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,10,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,11,21],[12,1,12,21],[13,1,13,21]],"flags":["formulas_cached_only"]}
["（一）煤炭行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴采矿","⑵露采","⑶选煤","⑷矿山机电","⑸机械","⑹电力","⑺电气","⑻建筑","⑼结构","⑽给排水","⑾暖通空调","⑿环保","⒀总图","⒁运输","⒂技术经济",null,null,"总计","备   注"]
[{"$nulls":3},"采矿矿物〔采矿〕","采矿矿物〔采矿〕","采矿矿物〔矿物加工〕",null,"机械",null,"电气〔供配电〕","建筑〔二级及以上〕","结构〔一级〕","公用设备〔给水排水〕","公用设备〔暖通空调〕","环保"]
["行业\n资质","甲级",null,7,5,4,2,3,1,3,2,3,1,1,1,1,2,2,null,null,38]
[null,"乙级",null,4,3,2,1,2,null,2,1,2,1,1,1,1,1,1,null,null,23]
["专业\n资质","矿井","甲级",7,null,null,2,2,1,3,2,3,1,1,1,1,2,2,null,null,28]
[null,null,"乙级",4,null,null,1,2,1,2,1,2,1,1,1,1,1,1,null,null,19]
[null,"露天矿","甲级",null,5,1,null,2,1,3,2,3,1,1,1,1,2,2,null,null,25]
[null,null,"乙级",null,3,null,null,1,null,2,1,2,1,1,1,1,1,1,null,null,15]
[null,"选煤厂","甲级",null,null,4,null,2,null,3,1,2,1,1,1,1,2,2,null,null,20]
[null,null,"乙级",null,null,2,null,1,null,2,1,1,1,1,1,1,1,1,null,null,13]
["注：","    1、专业设置中，工艺专业包括采矿、露采、选煤、矿山机电、机械。采矿包括采煤、矿建和通风安全；矿山机电包括提升、通风、排水、压风及井下运输；电气包括供配电、自动控制、通讯和信号；运输包括铁路、道路、桥涵。"]
[null,"    2、注册类型中，露采专业对应的注册采矿/矿物工程师（采矿）要求所学专业为露采专业或从事露采工程设计十年以上的主要专业技术人员。"]
[null,"    3、矿井设计类型中包括煤炭地下气化、瓦斯抽采集利用；选煤厂设计类型中包括水煤（焦）浆厂、型煤厂。"]

{"sheet":"(一)煤炭（2）","index":3,"n_rows":5,"n_cols":7,"rows_kept":5,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["（一）煤炭行业建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"矿井","万吨/年","≥120","90～45","≤30"]
[2,"露天矿","万吨/年","＞400","400～100","＜100"]
[3,"选煤厂","万吨/年","≥120","90～45","≤30"]

{"sheet":"（二）化工石化医药（1） ","index":4,"n_rows":31,"n_cols":22,"rows_kept":31,"merged":[[0,0,0,21],[1,0,2,2],[1,20,2,20],[1,21,2,21],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,14,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,12,1],[13,1,14,1],[17,0,22,0],[17,1,18,1],[19,1,20,1],[21,1,22,1],[23,1,23,21],[24,1,24,21],[25,1,25,21],[26,1,26,21],[27,1,27,21]],"flags":["formulas_cached_only"]}
["（二）化工石化医药行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴工艺","⑵建筑","⑶结构","⑷设备","⑸自控","⑹总图运输","⑺给排水","⑻暖通空调","⑼动力","⑽电气","⑾通信","⑿环保","⒀技术经济","⒁概预算",{"$nulls":3},"总计","备   注"]
[{"$nulls":3},"化工","建筑〔一级、二级〕","结构〔一级、二级〕","机械",null,null,"公用设备〔给排水〕","公用设备〔暖通〕","公用设备〔动力〕","电气",null,null,"造价"]
["行业\n资质","甲级",null,12,1,4,5,3,2,2,2,2,2,1,1,2,1,{"$nulls":3},40]
[null,"乙级",null,8,1,2,3,2,1,2,1,1,1,1,1,1,1,{"$nulls":3},26]
["专业\n资质","炼油\n工程","甲级",8,1,3,4,2,1,2,1,2,1,1,1,1,1,{"$nulls":3},29]
[null,null,"乙级",5,1,2,2,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},20]
[null,"化工\n工程","甲级",8,1,3,4,2,1,2,1,2,1,1,1,1,1,{"$nulls":3},29]
[null,null,"乙级",5,1,2,2,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},20]
[null,"石油及\n化工产\n品储运","甲级",4,1,2,3,2,1,1,1,2,1,1,1,1,1,{"$nulls":3},22]
[null,null,"乙级",2,1,2,2,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},17]
[null,"化工\n矿山","甲级",6,1,2,2,1,1,2,1,1,1,1,1,1,1,{"$nulls":3},22]
[null,null,"乙级",3,1,2,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},17]
[null,"生化\n生物","甲级",6,1,2,2,2,1,1,2,2,1,1,1,1,1,{"$nulls":3},24]
[null,null,"乙级",4,1,2,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},18]
[]
[{"$nulls":11},15]
["专业\n资质","中成药","甲级",5,1,2,2,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},20]
[null,null,"乙级",3,1,2,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},17]
[null,"药物\n制剂","甲级",6,1,2,2,2,1,1,2,2,1,1,1,1,1,{"$nulls":3},24]
[null,null,"乙级",4,1,2,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},18]
[null,"医药\n器械","甲级",3,1,2,4,1,1,1,1,1,2,1,1,1,1,{"$nulls":3},21]
[null,null,"乙级",2,1,1,3,1,1,1,1,1,1,1,1,1,1,{"$nulls":3},17]
["注：","1、石油及化工产品储运专业资质中，工艺专业人员可以是注册化工工程师或注册石油/天然气工程师。"]
[null,"2、行业甲、乙级资质和专业甲级资质要求建筑专业人员为一级注册建筑师，专业乙级资质可以是二级注册建筑师。"]
[null,"3、行业甲、乙级资质和专业甲级资质要求结构专业人员为一级注册结构工程师，专业乙级资质可以是二级注册结构工程师。"]
[null,"4、化工矿山专业资质工艺专业人员应是注册采矿/矿物工程师。"]
[]
[]
[]
[{"$nulls":11},16]

{"sheet":"（二）化工石化医药（2） ","index":5,"n_rows":90,"n_cols":9,"rows_kept":90,"merged":[[0,0,0,8],[1,1,1,3],[2,0,14,0],[2,1,14,1],[2,2,2,3],[15,0,26,0],[15,1,26,1],[15,2,23,2],[24,2,26,2],[27,0,51,0],[27,1,51,1],[27,2,51,2],[42,3,43,3],[42,4,43,4],[52,0,64,0],[52,1,64,1],[52,2,56,2],[57,2,63,2],[64,2,64,3],[65,0,74,0],[65,1,74,1],[65,2,66,3],[67,2,68,3],[69,2,74,2],[69,3,70,3],[73,3,74,3],[75,0,78,0],[75,1,78,1],[75,2,78,2],[75,3,76,3],[77,3,78,3],[79,0,80,0],[79,1,80,1],[79,2,79,3],[80,2,80,3],[81,1,81,3],[82,1,82,3],[83,0,84,0],[83,1,83,3],[84,1,84,3],[85,1,85,3],[87,1,87,8],[88,1,88,8],[89,1,89,8]],"flags":["formulas_cached_only"]}
["（二）化工石化医药行业建设项目设计规模划分表"]
["序号","建设项目",null,null,"计量（算）单位","大型","中型","小型","备注"]
[1,"炼油工程","常减压蒸馏",null,"万吨/年","≥500","≥250"]
[{"$nulls":3},"气体分馏","万吨/年","≥30","≥15"]
[{"$nulls":3},"催化反应加工","万吨/年","≥200","≥120"]
[{"$nulls":3},"加氢裂化","万吨/年","≥140","≥80"]
[{"$nulls":3},"加氢精制","万吨/年","≥200","≥100"]
[{"$nulls":3},"制氢","万标立方米/时","≥6","≥4"]
[{"$nulls":3},"气体脱硫","万吨/年","≥30","≥10"]
[{"$nulls":3},"液化气脱硫","万吨/年","≥60","≥30"]
[{"$nulls":3},"制硫","万吨/年","≥10","≥6"]
[{"$nulls":3},"焦化","万吨/年","≥140","≥100"]
[{"$nulls":3},"气体加工","万吨/年","≥10","≥6"]
[{"$nulls":3},"润滑油加氢","万吨/年","≥30","≥ 15"]
[{"$nulls":3},"重整装置","万吨/年","≥60","≥40"]
[2,"化工工程","无机化工","合成氨","万吨/年","> 18","8～18"]
[{"$nulls":3},"尿素","万吨/年","> 30","13 ～30"]
[{"$nulls":3},"硫酸","万吨/年","> 16","8 ～16"]
[{"$nulls":3},"磷酸","万吨/年","> 12","3～12"]
[{"$nulls":3},"烧碱","万吨/年","> 5","3 ～5"]
[{"$nulls":3},"纯碱","万吨/年","> 30","8～30"]
[{"$nulls":3},"磷肥 \n(普钙、钙镁磷肥)","万吨/年","> 50","20～ 50"]
[{"$nulls":3},"复肥","万吨/年","> 20","10 ～20"]
[{"$nulls":3},"无机盐","亿元"," > 1","0.5～1"]
[null,null,"有机化工","乙烯","万吨/年","≥30","14～30"]
[{"$nulls":3},"对二甲苯（PX）","万吨/年","≥15","5～15"]
[{"$nulls":3},"丁二烯","万吨/年","≥5","＜5"]
[2,"化工工程","有机化工","乙二醇","万吨/年","≥10","＜10"]
[{"$nulls":3},"精对苯二甲酸（PTA）","万吨/年","≥25","15 ～25"]
[{"$nulls":3},"醋酸乙烯","万吨/年","≥8","＜8"]
[{"$nulls":3},"甲醇","万吨/年","≥10","5 ～10"]
[{"$nulls":3},"氯乙烯","万吨/年","≥8","＜8"]
[{"$nulls":3},"苯乙烯","万吨/年","≥10","＜10"]
[{"$nulls":3},"醋酸","万吨/年","≥10","＜10"]
[{"$nulls":3},"环氧丙烷","万吨/年","≥4","＜4"]
[{"$nulls":3},"苯酐","万吨/年","≥4","＜4"]
[{"$nulls":3},"苯酚丙酮","万吨/年","≥6","＜6"]
[{"$nulls":3},"丙烯腈","万吨/年","≥5","＜5"]
[{"$nulls":3},"低密度聚乙烯","万吨/年","≥18","＜18"]
[{"$nulls":3},"高密度聚乙烯","万吨/年","≥14","＜14"]
[{"$nulls":3},"全密度聚乙烯","万吨/年","≥14","＜14"]
[{"$nulls":3},"聚苯乙烯","万吨/年","≥10","＜10"]
[{"$nulls":3},"聚氯乙烯","万吨/年","≥10","＜10",null,"乙烯法"]
[{"$nulls":5},"≥5","＜5",null,"电石法"]
[{"$nulls":3},"聚乙烯醇","万吨/年","≥6","＜6"]
[{"$nulls":3},"己内酰胺","万吨/年","≥6","＜6"]
[{"$nulls":3},"聚脂","万吨/年","≥10","＜10"]
[{"$nulls":3},"尼龙66","万吨/年","≥5","＜5"]
[{"$nulls":3},"聚丙烯","万吨/年","≥7","＜7"]
[{"$nulls":3},"ABS","万吨/年","≥10","＜10"]
[{"$nulls":3},"顺丁橡胶","万吨/年","≥5","＜5"]
[{"$nulls":3},"丁苯橡胶","万吨/年","≥5","＜5"]
[2,"化工工程","有机化工","丁基橡胶","万吨/年","≥3"]
[{"$nulls":3},"乙丙橡胶","万吨/年",null,"≥2"]
[{"$nulls":3},"丁腈橡胶","万吨/年",null,"≥1"]
[{"$nulls":3},"高效低毒农药","吨/年","≥1000","500～1000"]
[{"$nulls":3},"精细化工","亿元","≥0.5","0.3～ 0.5"]
[null,null,"合成材料及加工","树脂成型加工","万吨/年","≥3","1 ～3"]
[{"$nulls":3},"塑料薄膜","万吨/年","≥0.3","0.1～0.3"]
[{"$nulls":3},"化纤（长丝、短丝、无纺布、特种纤维等）","万吨/年","≥9","≥3"]
[{"$nulls":3},"塑料编织袋","万条/年","≥500","＜500"]
[{"$nulls":3},"油漆及涂料（不含高档油漆）","万吨/年","≥4","1 ～4"]
[{"$nulls":3},"橡胶轮胎工程","万套/年","≥30","10 ～30"]
[{"$nulls":3},"其他橡胶制品","亿元","≥0.5","＜0.5"]
[null,null,"其它石油化工项目",null,"亿元","≥3","1 ～3"]
[3,"石油及化工产品储运","输油",null,"万吨/年","≥600","≥ 300",null,"能力"]
[{"$nulls":4},"公里","≥120","30 ～ 120",null,"长度"]
[null,null,"输气",null,"亿立方米/年","≥2.5","≥1",null,"能力"]
[{"$nulls":4},"公里","≥120","30 ～120",null,"长度"]
[null,null,"油库","①原油","万立方米","≥20","≥8",null,"总容积"]
[{"$nulls":4},"万立方米","≥5","    ≥2    ",null,"单罐容积"]
[{"$nulls":3},"②成品油","万立方米","≥8","≥3",null,"总容积"]
[{"$nulls":3},"②成品油","万立方米","≥2","≥1",null,"单罐容积"]
[{"$nulls":3},"③天然气","万立方米","≥1.5"," ≥ 1",null,"总容积"]
[{"$nulls":4},"万立方米","≥0.5","   ≥0.1 ",null,"单罐容积"]
[3,"石油及化工产品储运","油库","④常温液化石油气","立方米","≥2000","≥1000",null,"总容积"]
[{"$nulls":4},"立方米","≥400","≥200",null,"单罐容积"]
[{"$nulls":3},"⑤低温液化石油气","万立方米","≥2","≥1",null,"总容积"]
[{"$nulls":4},"万立方米","≥1","≥0.5",null,"单罐容积"]
[4,"化工矿山","磷矿",null,"万吨/年","≥100","30 ～100"]
[null,null,"硫铁矿",null,"万吨/年","≥100","30 ～100"]
[5,"生化、生物药",null,null,"亿元","≥1","0.5 ～1",null,"综合项目"]
[6,"中成药",null,null,"亿元","≥0.8","0.5 ～0.8",null,"综合项目"]
[7,"药物制剂",null,null,"亿元","≥1","0.5～ 1",null,"综合项目"]
[null,"化学原料药",null,null,"亿元","≥2","1～ 2",null,"综合项目"]
[8,"医疗器械",null,null,"亿元","≥0.8","0.3 ～0.8",null,"综合项目"]
[]
["注：","1、本表炼油及化工工程项目系指新建项目，改扩建项目除按此表核定规模外，还需核定工程投资，大型项目≥1.2亿元,中型项目≥0.8亿元。"]
[null,"2、石油及化工产品储运类别中，油气输送能力与长度是并列关系，油库总容积与单罐容积是并列关系。"]
[null,"3、因医药品种繁多、产量相差很大，所以医药建设项目以投资划分规模。申请设计资质时，业绩必须写清楚项目名称、产品品种、产量及投资。"]

{"sheet":"（三）石油天然气（1）","index":6,"n_rows":23,"n_cols":22,"rows_kept":23,"merged":[[0,0,0,21],[1,0,2,2],[1,20,2,20],[1,21,2,21],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,12,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,12,1],[11,21,12,21],[13,0,18,0],[13,1,14,1],[15,1,16,1],[17,1,18,1],[19,1,19,21],[20,1,20,21],[21,1,21,21],[22,1,22,21]],"flags":["formulas_cached_only"]}
["（三）石油天然气（海洋石油）行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴油气集输","⑵油气储运","⑶油气加工","⑷建筑","⑸结构","⑹总图","⑺给排水","⑻机械","⑼电气","⑽仪表自控\n及通信","⑾热力工程","⑿腐蚀与控制","⒀工程经济",{"$nulls":4},"总计","备   注"]
[{"$nulls":3},"石油天然气 ","石油天然气 ","石油天然气 ","建筑〔一级〕","结构〔一级〕",null,"公用设备〔给水排水〕","机械","电气〔发输变〕",null,"公用设备〔动力暖通空调〕",null,"造价"]
["行业\n资质","甲级",null,7,10,7,1,3,2,2,4,3,4,3,1,2,{"$nulls":4},49]
[null,"乙级",null,5,8,5,1,2,1,1,2,2,2,2,1,1,{"$nulls":4},33]
["专业\n资质","油田\n地面","甲级",7,4,null,1,3,2,2,3,3,2,2,1,1,{"$nulls":4},31]
[null,null,"乙级",5,2,null,1,2,1,2,2,2,2,2,1,1,{"$nulls":4},23]
[null,"气田\n地面","甲级",7,4,null,1,3,2,2,3,3,2,2,1,1,{"$nulls":4},31]
[null,null,"乙级",5,2,null,1,2,1,2,2,2,2,2,1,1,{"$nulls":4},23]
[null,"管道\n输送","甲级",null,10,null,1,3,1,2,1,2,4,2,1,2,{"$nulls":4},29]
[null,null,"乙级",null,5,null,1,2,1,1,1,1,2,1,1,1,{"$nulls":4},17]
[null,"海洋\n石油","甲级",4,4,2,null,5,2,2,3,2,2,1,1,2,{"$nulls":4},30,"要求结构专业为注册海洋工程师"]
[null,null,"乙级",2,2,1,null,2,1,1,2,1,1,1,1,1,{"$nulls":4},16]
["专业\n资质","油气库","甲级",null,5,null,1,3,1,2,4,2,2,2,1,2,{"$nulls":4},25]
[null,null,"乙级",null,2,null,1,2,1,1,2,1,2,2,1,1,{"$nulls":4},16]
[null,"油气\n加工","甲级",null,2,7,1,3,1,2,4,2,2,3,1,1,{"$nulls":4},29]
[null,null,"乙级",null,1,5,1,2,1,2,3,2,2,2,1,1,{"$nulls":4},23]
[null,"石油机\n械制造\n与修理","甲级",{"$nulls":3},1,3,1,2,5,2,2,2,null,1,{"$nulls":4},19]
[null,null,"乙级",{"$nulls":3},1,1,1,1,3,1,1,2,null,1,{"$nulls":4},12]
["注：","1、油气集输含注水、气、聚合物等及采出液处理。"]
[null,"2、热力工程包括热工和暖通。"]
[null,"3、乙级专业资质的注册建筑师为二级。"]
[null,"4、专业设置中关于结构专业只有海洋石油设计类型要求为注册海洋工程师，其他设计类型结构专业要求为结构一级注册工程师。"]

{"sheet":"（三）石油天然气（2）","index":7,"n_rows":27,"n_cols":8,"rows_kept":27,"merged":[[0,0,0,8],[1,1,1,2],[2,0,3,0],[2,1,3,2],[4,0,5,0],[4,1,5,2],[6,0,10,0],[6,1,10,1],[6,2,7,2],[8,2,9,2],[11,0,12,0],[11,1,12,1],[13,0,23,0],[13,1,23,1],[13,2,14,2],[15,2,16,2],[17,2,18,2],[19,2,20,2],[21,2,22,2],[24,0,25,0],[24,1,25,1],[26,1,26,2]],"flags":["formulas_cached_only"]}
["（三）石油天然气（海洋石油）行业建设项目设计规模划分表"]
["序号","建设项目",null,"计量（算）单位","大型","中型","小型","备注"]
[1,"油田\n地面工程",null,"万吨/年","≥30","30～20",null,"新建（产能）"]
[{"$nulls":3},"亿元","≥1","1～0.5",null,"技改\n（工程建设投资）"]
[2,"气田\n地面工程",null,"亿立方米/年","≥5","5～2",null,"新建（产能）"]
[{"$nulls":3},"亿元","≥1.5","1.5～0.5",null,"技改\n（工程建设投资）"]
[3,"管道\n输送\n工程","输油/浆体","万吨/年","≥600/≥500","600～300/\n500～200",null,"能力"]
[{"$nulls":3},"公里","≥200","200～100",null,"长度"]
[null,null,"输气","亿立方米/年","≥10","10～5",null,"能力"]
[{"$nulls":3},"公里","≥200","200～100",null,"长度"]
[null,null,"城镇燃气","亿立方米/年","≥3","3～1",null,"能力"]
[4,"海洋\n石油\n工程","海洋油气\n开发工程","亿元","≥8","8～4",null,"工程建设投资"]
[null,null,"海底管道工程","亿元","≥3","3～1",null,"工程建设投资"]
[5,"油气\n库工程","原油储库","万立方米","≥10","10～5",null,"总库容"]
[{"$nulls":3},"万立方米","≥5","5～2",null,"单罐容积"]
[null,null,"成品油库","万立方米","≥8","8～3",null,"总库容"]
[{"$nulls":3},"万立方米","≥2","2～0.5",null,"单罐容积"]
[null,null,"天然气\n储库","万立方米","≥1.5","1.5～1",null,"总库容"]
[{"$nulls":3},"万立方米","≥0.5","0.5～0.2",null,"单罐容积"]
[null,null,"液化气\n及轻烃\n储库","立方米","≥2000","2000～1000",null,"总库容"]
[{"$nulls":3},"立方米","≥400","400～200",null,"单罐容积"]
[null,null,"液化\n天然气\n储库 ","万立方米","≥12","12～6",null,"总库容"]
[{"$nulls":3},"万立方米","≥5","5～1",null,"单罐容积"]
[null,null,"地下储气库","亿立方米/年","≥3","3～1",null,"有效库容"]
[6,"油气\n加工\n工程 ","原油储库","万吨/年","≥30","30～20"]
[null,null,"天然气","万立方米/天","≥100","100～25"]
[7,"石油机械制造\n与修理工程",null,"亿元","≥0.5","0.5～0.2",null,"工程建设投资"]

{"sheet":"（四）电力（1）","index":8,"n_rows":20,"n_cols":32,"rows_kept":20,"merged":[[0,0,0,31],[1,0,2,2],[1,4,1,5],[1,7,1,8],[1,10,1,11],[1,12,1,13],[1,15,1,16],[1,30,2,30],[1,31,2,31],[3,0,4,0],[3,1,3,2],[3,31,4,31],[4,1,4,2],[5,0,13,0],[5,1,6,1],[7,1,9,1],[11,1,13,1],[14,0,16,0],[14,1,16,1],[17,1,17,31],[18,1,18,31],[19,1,19,31]],"flags":["formulas_cached_only"]}
["（四）电力行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴动力","⑵电气",null,"⑶建筑","⑷结构",null,"⑸给排水","⑹规划",null,"⑺地质",null,"⑻水工","⑼水土保持",null,"⑽征地移民","⑾工程施工","⑿环境保护","⒀水工建筑物监测","⒁水力/风力机械及金属结构","⒂水文气象","⒃工程经济及概预算","⒄输煤除灰","⒅电力系统","⒆热工控制","⒇通信保护","(21)化学水处理","(22)总图","总计","备   注"]
[{"$nulls":3},"公用设备〔动力〕","电气〔发输电〕",null,"建筑","结构","结构","公用设备〔给水排水〕","水利水电〔规划〕",null,"水利水电〔地质〕",null,"水利水电〔水工〕","水利水电〔水土保持〕",null,"水利水电〔征地移民〕"]
["行业\n资质","甲级",null,6,"10(2)",null,2,4,null,1,{"v":-4,"d":"(4)"},null,{"v":-4,"d":"(4)"},null,"2(8)",{"v":-2,"d":"(2)"},null,{"v":-3,"d":"(3)"},{"v":-4,"d":"(4)"},{"v":-2,"d":"(2)"},{"v":-2,"d":"(2)"},{"v":-4,"d":"(4)"},null,"2(3)",2,2,2,2,1,2,"38\n（38）","括号内数字为水力发电的主要专业技术人员配备。                     火力发电工程设计，水工可配置非注册专业人员。   "]
[null,"乙级",null,3,"6(2)",null,1,2,null,1,{"v":-2,"d":"(2)"},null,{"v":-2,"d":"(2)"},null,"1(4)",{"v":-1,"d":"(1)"},null,{"v":-1,"d":"(1)"},{"v":-2,"d":"(2)"},{"v":-1,"d":"(1)"},{"v":-1,"d":"(1)"},{"v":-2,"d":"(2)"},1,"2(2)",1,1,1,1,1,1,"23\n（20）"]
["专业\n资质","火力发电\n（含核电常规岛）","甲级",6,10,null,2,4,null,1,{"$nulls":4},2,{"$nulls":8},2,2,2,2,2,1,2,38,"水工可配置非注册专业人员"]
[null,null,"乙级",3,6,null,1,2,null,1,{"$nulls":4},1,{"$nulls":8},2,1,1,1,1,1,1,22,"水工可配置非注册专业人员"]
[null,"水力发电\n（含抽水蓄能、潮汐）","甲级",null,2,{"$nulls":5},4,null,4,null,8,2,null,3,4,2,2,4,null,3,{"$nulls":6},38]
[null,null,"乙级",null,2,{"$nulls":5},2,null,2,null,4,1,null,1,2,1,1,2,null,2,{"$nulls":6},20]
[null,null,"丙级",null,null,1,null,null,1,null,null,1,null,1,null,null,1,null,null,1,null,1,1,1,{"$nulls":6},9]
[null,"新能源","乙级",null,2,null,null,1,{"$nulls":13},1,1,1,{"$nulls":5},1,7,"注册结构师为二级"]
[null,"送电\n工程","甲级",null,5,null,null,2,{"$nulls":15},2,{"$nulls":3},2,null,null,11]
[null,null,"乙级",null,2,null,null,1,{"$nulls":15},1,{"$nulls":3},1,null,null,5]
[null,null,"丙级",null,null,1,null,null,1,{"$nulls":14},1,{"$nulls":6},3]
["专业\n资质","变电        工程","甲级",null,6,null,1,2,null,1,{"$nulls":13},2,null,2,{"$nulls":3},1,15,"注册建筑师为二级，\n给排水可配置非注册专业人员"]
[null,null,"乙级",null,3,null,1,1,null,1,{"$nulls":13},1,null,1,{"$nulls":3},1,9,"注册建筑师、结构工程师为二级，给排水可配置非注册专业人员"]
[null,null,"丙级",null,null,1,null,null,1,{"$nulls":14},1,{"$nulls":6},3]
["注：","1、同时具备发电专业（火力发电或水力发电）及送电专业工程设计资质，即可申请电力全行业工程设计资质。。"]
[null,"2、新能源（含风力、太阳能、地热、垃圾、秸秆发电），设计资质不设级别。垃圾、秸秆发电设计资质主要专业技术人员配备参照火力发电乙级标准。"]
[null,"3、核电常规岛只设甲级。"]

{"sheet":"（四）电力（2）","index":9,"n_rows":7,"n_cols":7,"rows_kept":7,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["（四）电力行业建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"火力发电","MW","≥100","50～25","≤25","单机容量"]
[2,"水力发电","MW","≥250","250～25","≤25"]
[3,"风力发电","MW","≥10","10～3","≤3"]
[4,"变电工程","KV","≥330","220～110","≤110"]
[5,"送电工程","KV","≥330","220～110","≤110"]

{"sheet":"（五）冶金（1）","index":10,"n_rows":13,"n_cols":24,"rows_kept":13,"merged":[[0,0,0,23],[1,0,2,2],[1,22,2,22],[1,23,2,23],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,12,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,12,1]],"flags":["formulas_cached_only"]}
["（五）冶金行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴金属冶炼","⑵金属材料加工","⑶焦化","⑷耐火","⑸采矿","⑹选矿","⑺建筑","⑻结构","⑼总图","⑽机械","⑾电力 ","⑿给排水","⒀暖通空调","⒁动力","⒂自动控制","⒃环境保护","⒄技术经济","⒅概预算",null,"总计","备   注"]
[{"$nulls":3},"冶金","冶金","冶金","冶金","采矿矿物〔采矿〕","采矿矿物〔矿物加工〕 ","建筑〔一级〕","结构〔一级〕",null,"机械","电气","公用设备〔给水排水〕","公用设备〔暖通空调〕","公用设备〔动力〕",null,"环保"]
["行业\n资质","甲级",null,10,10,{"$nulls":4},2,4,1,2,2,2,1,3,2,2,2,2,null,45]
[null,"乙级",null,5,5,{"$nulls":4},1,2,1,1,2,1,1,2,1,1,1,1,null,25]
["专业\n资质","金属冶炼工程","甲级",10,{"$nulls":5},2,4,1,2,2,2,1,3,2,2,2,2,null,35]
[null,null,"乙级",5,{"$nulls":5},1,2,1,1,2,1,1,2,1,1,1,1,null,20]
[null,"金属材料加工工程","甲级",null,10,{"$nulls":4},2,4,1,2,2,2,1,3,2,2,2,2,null,35]
[null,null,"乙级",null,5,{"$nulls":4},1,2,1,1,2,1,1,2,1,1,1,1,null,20]
[null,"焦化耐火工程","甲级",null,null,8,2,null,null,1,2,1,2,2,2,1,2,1,2,2,2,null,30]
[null,null,"乙级",null,null,4,1,null,null,1,2,1,1,1,1,1,1,1,1,1,1,null,18,"若为二级注册建筑师则需2名；二级注册结构工程师则需4名。"]
[null,"冶金矿山工程","甲级",1,{"$nulls":3},5,5,1,2,1,2,2,2,1,1,1,2,2,2,null,30,"黄金矿山含黄金冶炼"]
[null,null,"乙级",{"$nulls":4},2,2,1,2,null,1,1,1,1,1,null,1,1,1,null,15,"黄金矿山含黄金冶炼；若为二级注册建筑师则需2名；二级注册结构工程师则需4名。"]

{"sheet":"（五）冶金（2）","index":11,"n_rows":60,"n_cols":9,"rows_kept":60,"merged":[[0,0,0,8],[1,1,1,3],[2,0,24,0],[2,1,24,1],[2,2,3,3],[2,8,24,8],[4,2,7,2],[4,3,5,3],[6,3,7,3],[8,2,8,3],[8,5,8,6],[9,2,9,3],[10,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[16,2,16,3],[17,2,17,3],[18,2,20,2],[21,2,21,3],[22,2,22,3],[23,2,23,3],[24,2,24,3],[24,5,24,7],[25,0,42,0],[25,1,42,1],[25,2,27,3],[25,4,27,4],[25,8,45,8],[28,2,28,3],[29,2,29,3],[30,2,31,3],[30,4,31,4],[32,2,33,3],[32,4,33,4],[34,2,35,3],[34,4,35,4],[36,2,39,2],[40,2,42,2],[43,0,45,0],[43,1,45,1],[43,2,44,3],[45,2,45,3],[46,0,49,0],[46,1,49,1],[46,2,46,3],[46,8,59,8],[47,2,47,3],[48,2,48,3],[49,2,49,3],[50,0,58,0],[50,1,58,1],[50,2,51,3],[52,2,52,3],[53,2,53,3],[54,2,54,3],[55,2,55,3],[56,2,56,3],[57,2,57,3],[58,2,58,3],[59,1,59,3]],"flags":["formulas_cached_only"]}
["（五）冶金行业建设项目设计规模划分表"]
["序号","建设项目",null,null,"计量（算）单位","大型","中型","小型","备注"]
[1,"金属冶炼工程","炼铁",null,"万吨铁/年","≥100","＜100～50","无"]
[{"$nulls":4},"或单座高炉炉容        立方米","≥1000","＜1000～300","无"]
[null,null,"炼钢","转炉","万吨钢/年","≥100","＜100～50","无"]
[{"$nulls":4},"或单座转炉公称容量吨","≥120","＜120～30","无"]
[{"$nulls":3},"电炉","万吨钢/年","≥100","＜100～50","无"]
[{"$nulls":4},"或单座电炉公称容量吨","≥70","＜70～20","无"]
[null,null,"炉外精炼与连铸",null,null,"与炼铁匹配",null,"无"]
[null,null,"铁合金",null,"单座还原电炉能力KVA","≥25000","＜25000～12500","无"]
[null,null,"烧结",null,"万吨烧结矿/年","≥200","＜200～100","无"]
[{"$nulls":4},"或单台烧结机规格   平方米","≥180","＜180～90","无"]
[null,null,"带式焙烧、链蓖机回转窑球团",null,"万吨球团矿/年","≥200","＜200～100","无"]
[null,null,"竖炉球团",null,"平方米/单座","≥16","＜16～8","＜8"]
[null,null,"氧化铝厂",null,"万吨/年","＞60","≤60～30","＜30"]
[null,null,"电解铝厂",null,"万吨/年","≥20","＜20～5","＜5"]
[null,null,"镁厂",null,"万吨/年","≥1.0","＜1.0～0.5","＜0.5"]
[null,null,"钛厂（海绵钛）",null,"万吨/年","≥1.0","＜1.0～0.3","＜0.3"]
[null,null,"炭素厂","电极","万吨/年","≥2.0","＜2.0～1.0","＜1.0"]
[{"$nulls":3},"阴极","万吨/年","≥2.0","＜2.0～1.0","＜1.0"]
[{"$nulls":3},"阳极","万吨/年","≥12","＜12～3","＜3"]
[null,null,"镍联合企业",null,"万吨镍/年","≥3","＜3～1","＜1"]
[null,null,"其他重金属            联合企业",null,"万吨金属/年","≥5","＜5～3","＜3"]
[null,null,"常用金属冶炼、    电解厂",null,"万吨金属/年","≥5","＜5～3","＜3"]
[null,null,"黄金",null,"万吨/年","与矿山规模匹配 "]
[2,"金属材料加工工程","板带轧钢",null,"宽度毫米","≥2800\n中厚板轧机","＜2800～2300\n中厚板轧机","无"]
[{"$nulls":5},"或≥800\n冷轧、热轧、涂镀层机组","＜800","无"]
[{"$nulls":5},"或≥1200\n单机架冷轧机","＜1200","无"]
[null,null,"型钢轧钢",null,"辊径毫米","≥750\n型钢轧机；或连续式或半连续式大、中、小型型材轧机","＜750 型钢轧机","无"]
[null,null,"线材轧机",null,"速度米/秒","≥50连续式线材轧机","＜50","无"]
[null,null,"钢管轧机",null,"直径毫米","≥114钢管轧机","＜114","无"]
[{"$nulls":5},"≥168焊管轧机 ","＜168","无"]
[null,null,"精、快锻",null,"锻造压力吨","≥1000精锻","＜1000","无"]
[{"$nulls":5},"≥2000快锻","＜2000","无"]
[null,null,"金属制品",null,"万吨/年","≥1 一般钢丝及制品","＜1","无"]
[{"$nulls":5},"≥0.5 特殊钢丝及制品","＜0.5","无"]
[null,null,"重金属  加工","板带材","万吨/年","≥5","＜5～1","＜1"]
[{"$nulls":3},"管棒材","万吨/年","≥10","＜10～5","＜5"]
[{"$nulls":3},"电解铜箔","万吨/年","≥0.5","＜05～0.1","＜0.1"]
[{"$nulls":3},"线杆","万吨/年","≥15","＜15～8","＜8"]
[null,null,"轻金属\n加工","板带箔材","万吨/年","≥10","＜10～3","＜3"]
[{"$nulls":3},"型材","万吨/年","≥6","＜6～2","＜2"]
[{"$nulls":3},"双零箔材","万吨/年","≥1","＜1～0.3","＜0.3"]
[3,"焦化耐火工程","炼焦",null,"万吨焦炭/年","≥100","＜100～60","无"]
[{"$nulls":4},"米","或炭化室高度≥6","＜6～4.3 ","无"]
[null,null,"焦化产品",null,"万立方米/小时","焦炉煤气净化能力≥5","＜5～3","无"]
[3,"焦化耐火工程","焦化产品",null,"万吨/年","焦油加工能力≥15；粗笨精制能力≥5","焦油加工能力   ＜15～10；粗笨精制能力＜5～2.5","无"]
[null,null,"普通\n耐火材料",null,"万吨/年","粘土砖、硅砖≥2或\n其他耐火砖≥1","粘土砖、硅砖＜2或\n其他耐火砖＜1","无"]
[null,null,"新型高级和           功能耐火材料",null,"万吨/年","高纯镁砂≥1；或优质高纯铝矾土≥10，或其他耐火材料≥0.1","高纯镁砂＜1；或优质高纯铝矾土＜10，或其他耐火材料＜0.1","无"]
[null,null,"活性石灰 ",null,"万吨/年","≥5","＜5","无"]
[4,"冶金矿山工程","露天铁矿采矿",null,"万吨矿石/年","≥200","＜200～60","＜60"]
[{"$nulls":4},"万吨矿岩/年","≥1000","＜1000～300","＜300"]
[null,null,"地下铁矿采矿",null,"万吨矿石/年","≥100","＜100～30","＜30"]
[null,null,"铁矿选矿",null,"万吨矿石/年","≥200","＜200～60","＜60"]
[null,null,"砂矿采、选",null,"万吨矿石/年","≥200","≤200～100","＜100"]
[null,null,"脉矿采、选",null,"万吨矿石/年","≥100","≤100～20","＜20"]
[null,null,"岩金矿采、选",null,"吨原矿/日","≥500","＜500～100","＜100"]
[null,null,"砂金矿采、选",null,"采金船斗容（升）","≥500","＜500"]
[null,null,"砂金矿露天采、选",null,"立方米砂金矿/小时","≥320","＜320～160","＜160"]
[5,"其他冶金工程",null,null,"投资万元","≥20000","＜20000～5000","＜5000"]

{"sheet":"（六）军工（1）","index":12,"n_rows":44,"n_cols":34,"rows_kept":44,"merged":[[0,0,0,33],[1,0,2,2],[1,32,2,32],[1,33,2,33],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,8,0],[5,1,6,1],[7,1,8,1],[9,0,14,0],[9,1,10,1],[11,1,12,1],[13,1,14,1],[15,0,20,0],[15,1,16,1],[17,1,18,1],[19,1,20,1],[21,0,26,0],[21,1,22,1],[23,1,24,1],[25,1,26,1],[27,0,32,0],[27,1,28,1],[29,1,30,1],[31,1,32,1],[33,0,38,0],[33,1,34,1],[35,1,36,1],[37,1,38,1],[39,0,40,0],[39,1,40,1],[41,1,41,33],[42,1,42,33],[43,1,43,33]],"flags":["formulas_cached_only"]}
["（六）军工行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴导弹及火箭弹","⑵弹、火工品及固体发动机","⑶燃机、动力装置及航天发动机","⑷控制系统、光学、光电、电子、仪表","⑸科研、靶场、试验、教育、培训","⑹地面设备","⑺航天空间飞行器","⑻运载火箭","⑼地面制导站","⑽航空飞行器","⑾机场工程","⑿船舶制造","⒀船舶机械","⒁船舶水工","⒂坦克、装甲车辆","⒃枪、炮","⒄火、炸药","⒅防化、民爆器材","⒆建筑","⒇结构","(21)总图","(22)给排水","(23)暖通","(24)动力","(25)电气〔自控〕","(26)概预算","(27)环保、〔安全、卫生〕",null,null,"总计","备   注"]
[{"$nulls":3},"航空航天军工","航空航天军工造船","航空航天军工造船","航空航天军工造船","航空航天军工造船","航空航天军工造船","航空航天","航空航天","航空航天","航空航天","航空航天","造船","造船","造船","军工","军工","军工","军工","建筑〔一级〕","结构〔一级〕","规划","公用设备〔给水排水〕","公用设备〔暖通空调〕","公用设备〔动力〕","电气","造价","环保"]
["行业\n资质","甲级",null,3,3,3,3,3,2,2,3,2,3,2,4,4,3,3,2,3,2,2,3,2,1,1,1,2,2,1,null,null,65]
[null,"乙级",null,2,2,2,2,2,1,1,2,1,2,1,3,3,2,2,1,2,1,1,2,1,1,1,1,2,1,1,null,null,43]
["专业\n资质","导弹及火箭弹工程","甲级",3,{"$nulls":17},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",2,{"$nulls":17},1,2,1,1,1,1,2,1,1,null,null,13]
[null,"弹、火工品及固体发动机\n工程","甲级",null,3,{"$nulls":16},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",null,2,{"$nulls":16},1,2,1,1,1,1,2,1,1,null,null,13]
["专业\n资质","燃机、动力装置及航天发动机工程","甲级",null,null,3,{"$nulls":15},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",null,null,2,{"$nulls":15},1,2,1,1,1,1,2,1,1,null,null,13]
[null,"控制系统、光学、光电、电子、仪表工程","甲级",{"$nulls":3},3,{"$nulls":14},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",{"$nulls":3},2,{"$nulls":14},1,2,1,1,1,1,2,1,1,null,null,13]
[null,"科研、靶场、试验、教育培训工程","甲级",{"$nulls":4},3,{"$nulls":13},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",{"$nulls":4},2,{"$nulls":13},1,2,1,1,1,1,2,1,1,null,null,13]
["专业\n资质","地面设备\n工程","甲级",{"$nulls":5},2,{"$nulls":12},2,3,2,1,1,1,2,2,1,null,null,17]
[null,null,"乙级",{"$nulls":5},1,{"$nulls":12},1,2,1,1,1,1,2,1,1,null,null,12]
[null,"航天空间         飞行器工程","甲级",{"$nulls":6},2,{"$nulls":11},2,3,2,1,1,1,2,2,1,null,null,17]
[null,null,"乙级",{"$nulls":6},1,{"$nulls":11},1,2,1,1,1,1,2,1,1,null,null,12]
[null,"运载火箭制造工程","甲级",{"$nulls":7},3,{"$nulls":10},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",{"$nulls":7},2,{"$nulls":10},1,2,1,1,1,1,2,1,1,null,null,13]
["专业\n资质","地面制导站\n工程","甲级",{"$nulls":8},2,{"$nulls":9},2,3,2,1,1,1,2,2,1,null,null,17]
[null,null,"乙级",{"$nulls":8},1,{"$nulls":9},1,2,1,1,1,1,2,1,1,null,null,12]
[null,"航空飞行器\n工程","甲级",{"$nulls":9},3,{"$nulls":8},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",{"$nulls":9},2,{"$nulls":8},1,2,1,1,1,1,2,1,1,null,null,13]
[null,"机场\n工程","甲级",{"$nulls":10},2,{"$nulls":7},2,3,2,1,1,1,2,2,1,null,null,17]
[null,null,"乙级",{"$nulls":10},1,{"$nulls":7},1,2,1,1,1,1,2,1,1,null,null,12]
["专业\n资质","船舶制造\n工程","甲级",{"$nulls":11},4,{"$nulls":6},2,3,2,1,1,1,2,2,1,null,null,19]
[null,null,"乙级",{"$nulls":11},3,{"$nulls":6},1,2,1,1,1,1,2,1,1,null,null,14]
[null,"船舶机械\n工程","甲级",{"$nulls":12},4,{"$nulls":5},2,3,2,1,1,1,2,2,1,null,null,19]
[null,null,"乙级",{"$nulls":12},3,{"$nulls":5},1,2,1,1,1,1,2,1,1,null,null,14]
[null,"船舶水工\n工程","甲级",{"$nulls":13},3,{"$nulls":4},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",{"$nulls":13},2,{"$nulls":4},1,2,1,1,1,1,2,1,1,null,null,13]
["专业\n资质","坦克、装甲     车辆工程","甲级",{"$nulls":14},3,{"$nulls":3},2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",{"$nulls":14},2,{"$nulls":3},1,2,1,1,1,1,2,1,1,null,null,13]
[null,"枪、炮\n工程","甲级",{"$nulls":15},2,null,null,2,3,2,1,1,1,2,2,1,null,null,17]
[null,null,"乙级",{"$nulls":15},1,null,null,1,2,1,1,1,1,2,1,1,null,null,12]
[null,"火、炸药\n工程","甲级",{"$nulls":16},3,null,2,3,2,1,1,1,2,2,1,null,null,18]
[null,null,"乙级",{"$nulls":16},2,null,1,2,1,1,1,1,2,1,1,null,null,13]
["专业\n资质","防化、民爆     器材工程","甲级",{"$nulls":17},2,2,3,2,1,1,1,2,2,1,null,null,17]
[null,null,"乙级",{"$nulls":17},1,1,2,1,1,1,1,2,1,1,null,null,12]
["注：","1、军工全行业甲级、乙级资质主要专业技术人员配备需至少同时满足6个设计类型人员配备要求即可。"]
[]
[null,"3、 军工行业和各专业设计资质不设丙级，专项设计资质目前暂不设立，今后视行业发展需求商建设部另行确定。"]

{"sheet":"（六）军工（2）","index":13,"n_rows":31,"n_cols":7,"rows_kept":31,"merged":[[0,0,0,6],[8,0,10,0],[8,1,10,1],[8,6,10,6],[11,0,13,0],[11,1,13,1],[11,6,13,6],[14,0,16,0],[14,1,16,1],[14,6,16,6],[17,0,18,0],[19,3,19,5],[20,0,21,0],[20,1,21,1]],"flags":["formulas_cached_only"]}
["（六）军工行业建设项目设计规模划分表"]
["序号","建设项目","计量(算)单位","大型","中型","小型","备注"]
[1,"导弹及火箭弹工程","万元",">3000","1000～3000","<1000","工程总投资"]
[2,"弹、火工品及固体发动机工程","万元",">3000","1000～3000","<1000","工程总投资"]
[3,"燃机、动力装置及航天发电机工程","万元",">3000","1000～3000","<1000","工程总投资"]
[4,"控制系统、光学、光电、电子、仪表工程","万元",">3000","1000～3000","<1000","工程总投资"]
[5,"科研、靶场、试验、教育培训工程","万元",">3000","1000～3000","<1000","工程总投资"]
[6,"地面设备工程","万元",">2000","1000～2000","<1000","工程总投资"]
[7,"航天空间飞行器","万元",">3000","1000～3000","<1000","工程总投资、面积或跨度；三项要求中有一个以上（含一个）达到大型标准，该项目即视为大型项目，同理类推"]
[null,null,"平方米",">3000","1000～3000","<1000"]
[null,null,"米",">18","12～18","<12"]
[8,"运载火箭","万元",">3000","1000～3000","<1000","工程总投资、面积或跨度；三项要求中有一个以上（含一个）达到大型标准，该项目即视为大型项目，同理类推"]
[null,null,"平方米",">3000","1000～3000","<1000"]
[null,null,"米",">18","12～18","<12"]
[9,"地面制导站","万元",">3000","1000～3000","<1000","工程总投资、面积或跨度；三项要求中有一个以上（含一个）达到大型标准，该项目即视为大型项目，同理类推"]
[null,null,"平方米",">3000","1000～3000","<1000"]
[null,null,"米",">18","12～18","<12"]
[10,"航空飞行器（综合）","万元",">10000","3000～10000","<3000","工程总投资"]
[null,"航空飞行器（单项）","万元",">3000","1000～3000","<1000","工程总投资"]
[11,"机场工程","万元",">10000",null,null,"工程总投资"]
[12,"船舶制造工程","万吨/年",">50","30～50","<30","年造船能力"]
[null,null,"万元",">20000","10000～20000","<10000","工程总投资"]
[13,"船舶科研工程","万元",">5000","3000～5000","<3000","工程总投资"]
[14,"船舶机械工程","万元",">5000","3000～5000","<3000","工程总投资"]
[15,"船舶水工工程","万元",">5000","3000～5000","<3000","工程总投资"]
[16,"坦克、装甲车辆","万元",">3000","1000～3000","<1000","工程总投资"]
[17,"枪","万元",">2000","1000～2000","<1000","工程总投资"]
[18,"炮","万元",">3000","1000～3000","<1000","工程总投资"]
[19,"炸药、火药","万元",">3000","1000～3000","<1000","工程总投资"]
[20,"防化器材","万元",">2000","1000～2000","<1000","工程总投资"]
[21,"民爆器材","万元",">2000","1000～2000","<1000","工程总投资"]

{"sheet":"（七）机械（1）","index":14,"n_rows":19,"n_cols":26,"rows_kept":19,"merged":[[0,0,0,25],[1,0,2,2],[1,24,2,24],[1,25,2,25],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,12,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,12,1],[13,0,16,0],[13,1,14,1],[15,1,16,1],[17,1,17,25],[18,1,18,25]],"flags":["formulas_cached_only"]}
["（七）机械行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴工艺","⑵建筑","⑶结构","⑷非标设备","⑸自控","⑹电气","⑺给排水","⑻暖通空调","⑼动力","⑽通信","⑾总图〔含物流〕\n","⑿经济","⒀概预算",{"$nulls":8},"总计","备   注"]
[{"$nulls":3},"机械","建筑〔一级〕","结构〔一级〕","机械",null,"电气〔供配电〕","公用设备〔给水排水〕","公用设备〔暖通空调〕","公用设备〔动力〕",null,null,"造价"]
["行业\n资质","甲级",null,12,2,4,1,1,2,2,2,1,1,1,1,{"$nulls":9},30]
[null,"乙级",null,7,1,2,null,null,1,1,1,null,null,1,null,1,{"$nulls":8},15]
["专业\n资质","通用设备制造业工程","甲级",9,2,4,1,1,2,2,2,1,1,1,1,{"$nulls":9},27]
[null,null,"乙级",5,1,2,null,null,1,1,1,null,null,1,null,1,{"$nulls":8},13]
[null,"专业设备制造业工程","甲级",9,2,4,1,1,2,2,2,1,1,1,1,{"$nulls":9},27]
[null,null,"乙级",5,1,2,null,null,1,1,1,null,null,1,null,1,{"$nulls":8},13]
[null,"交通运输设备    制造工程","甲级",9,2,4,1,1,2,2,2,1,1,1,1,{"$nulls":9},27]
[null,null,"乙级",5,1,2,null,null,1,1,1,null,null,1,null,1,{"$nulls":8},13]
[null,"电气机械设备  制造工程","甲级",9,2,4,1,1,2,2,2,1,1,1,1,{"$nulls":9},27]
[null,null,"乙级",5,1,2,null,null,1,1,1,null,null,1,null,1,{"$nulls":8},13]
["专业\n资质","金属制品业      工程","甲级",9,2,4,1,1,2,2,2,1,1,1,1,{"$nulls":9},27]
[null,null,"乙级",5,1,2,null,null,1,1,1,null,null,1,null,1,{"$nulls":8},13]
[null,"仪器仪表及文化办公机械制造业工程","甲级",9,2,4,1,1,2,2,2,1,1,1,1,{"$nulls":9},27]
[null,null,"乙级",5,1,2,null,null,1,1,1,null,null,1,null,1,{"$nulls":8},13]
["注：","1、机械行业专业资质划分为6类，其中每一类别含义见《国民经济行业分类》（GB/T4754-2002）。 "]
[null,"2、工艺专业是指冷加工（含机械加工、装配工具、机修、电修、计量、木工等专业），热加工（含铸造、锻造、热处理、冲压、焊接等专业），表处理（含电镀、涂装等专业）等专业。"]

{"sheet":"（七）机械（2）","index":15,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[4,0,4,6],[5,0,6,0],[5,1,6,1],[7,0,8,0],[7,1,8,1],[25,1,25,6]],"flags":["formulas_cached_only"]}
["（七）机械行业建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"机械厂项工程","万元",">5000","5000～2000","<2000","总投资额"]
[2,"机械单项工程","万元",">2000","2000～500","<500","总投资额"]
["以上类型中工业厂房的基本特征参数对照如下"]
[1,"单层工业厂房","吨",">30","30～15","≤15","吊车吨位"]
[null,null,"米",">24","24～18","≤18","跨度"]
[2,"多层工业厂房","米","＞12","≤12",null,"跨度"]
[null,null,"层","＞6","≤6",null,"层数"]
{"$rows_empty":16}
["注：","申报机械行业工程设计资质，按机械厂项工程的总投资额及相应工业厂房的基本特征参数来考核。"]

{"sheet":"（八）商物粮（1）","index":16,"n_rows":19,"n_cols":30,"rows_kept":19,"merged":[[0,0,0,29],[1,0,2,2],[1,28,2,28],[1,29,2,29],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,8,0],[5,1,6,1],[7,1,8,1],[9,0,14,0],[9,1,10,1],[11,1,12,1],[13,1,14,1],[15,0,16,0],[15,1,16,1],[17,1,17,29],[18,1,18,29]],"flags":["formulas_cached_only"]}
["（八）商物粮行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴制冷","⑵食品加工","⑶石油储运","⑷物流、仓储","⑸粮食工程","⑹油脂工程","⑺建筑","⑻结构","⑼暖通","⑽给排水","⑾电气","⑿自控","⒀总图","⒁概预算",{"$nulls":11},"总计","备   注"]
[{"$nulls":3},"公用设备",null,"公用设备",{"$nulls":3},"建筑〔一级、二级〕","结构〔一级、二级〕","公用设备〔暖通空调〕","公用设备〔给水排水〕","电气",null,null,"造价"]
["行业\n资质","甲级",null,"5　⑶",4,"2　　⑴",2,7,"4　　⑵","4　　⑵","5　　⑷","3　　⑵","3　　⑴","3　　⑵",2,2,"2　　⑴",{"$nulls":11},48,"⑺-⒁公用专业相同情况下，在⑴-⑹中任选两项"]
[null,"乙级",null,"3　　⑵",3,"1　　⑴　",1,4,"2　　⑴","3　　⑴","4　　⑵","2　　⑴","2　　⑴","2　　⑴",1,1,"2　　⑴",{"$nulls":11},31,"⑺-⒁公用专业相同情况下，在⑴-⑹中任选两项"]
["专业\n资质","冷冻冷藏工程","甲级","3  ⑵",{"$nulls":5},"2　　⑴","3　　⑴","2　　⑴","2　　⑴","2　　⑴",2,2,2,{"$nulls":11},20]
[null,null,"乙级","2　　⑴　",{"$nulls":5},"2　　①　","2　　⑴","1　　⑴",1,"1　　⑴",1,1,1,{"$nulls":11},12]
[null,"肉食品加工    工程","甲级","3　　⑵",2,{"$nulls":4},"2　　⑴","3　　⑴","2　　⑴",2,"2　　⑴",2,2,2,{"$nulls":11},22]
[null,null,"乙级","2　　⑴　",1,{"$nulls":4},"2　　①　","2　　⑴","1　　⑴",1,1,"1　　⑴",1,1,{"$nulls":11},13]
["专业\n资质","批发配送与物流仓储工程","甲级",{"$nulls":3},2,null,null,"2　⑴","3　　⑵","2　　⑴",2,"2　　⑴",2,2,2,{"$nulls":11},19]
[null,null,"乙级",{"$nulls":3},2,null,null,"2　　⑴","2　　⑴","1　　⑴",1,"1　　⑴",1,1,1,{"$nulls":11},12]
[null,"成品油储运    工程","甲级",null,null,"2　⑴",{"$nulls":3},"2  ⑴","2　　⑴",2,"2　　⑴","2　　⑴",2,2,2,{"$nulls":11},18]
[null,null,"乙级",null,null,"2　　⑴",{"$nulls":3},"1　　①","1　　⑴",1,"1　　⑴","1　　⑴",1,1,1,{"$nulls":11},10]
[null,"粮食    工程","甲级",{"$nulls":4},7,null,"2　　⑴","4　　⑵","2　　⑴",2,"3　　⑵",2,2,"2　　⑴",{"$nulls":11},26]
[null,null,"乙级",{"$nulls":4},4,null,"1　　⑴　","3　　⑴","1　　⑴",1,"2　　⑴",1,1,1,{"$nulls":11},15]
["专业      资质","油脂    工程","甲级",0,{"$nulls":4},"5　　⑵","2　　⑴",4,"2　　⑴",2,"3　　⑴　",2,2,"2　　⑴",{"$nulls":11},24]
[null,null,"乙级",0,{"$nulls":4},"3　　⑴","1　　①","3　　⑴","1　　⑴",1,"2　　⑴",1,1,1,{"$nulls":11},14]
["注：","（）内的数字为要求的注册人员数，其中建筑师和结构工程师为一级人员数；"]
[null,"  ○   内的数字为要求的二级注册建筑师和结构工程师人员数。"]

{"sheet":"（八）商物粮（2）","index":17,"n_rows":33,"n_cols":7,"rows_kept":33,"merged":[[0,0,0,6],[2,0,6,0],[7,0,12,0],[13,0,18,0],[19,0,20,0],[19,1,20,1],[21,0,26,0],[27,0,28,0],[29,0,32,0]],"flags":["formulas_cached_only"]}
["（八）商物粮行业建设项目设计规模划分表"]
["序号","项目名称","单位","大型","中型","小型","备注"]
[1,"冷冻冷藏库工程"]
[null,"1）冷藏库","m3","≥20000","20000~5000","<5000"]
[null,"2）气调库","m3","≥12000","12000~4000","<4000"]
[null,"3）制冰厂","吨/日","≥120","120~40","<40"]
[null,"4）果蔬加工","吨/小时","≥2","2~0.5","<0.5"]
[2,"肉食品加工工程"]
[null,"1）猪屠宰加工","头/班","≥2000","2000~1000","<1000"]
[null,"2）牛屠宰加工","头/班","≥150","150~50","<50"]
[null,"3）羊屠宰加工","头/班","≥3000","3000~1000","<1000"]
[null,"4）家禽屠宰加工","只/班","≥30000","30000~10000","<10000"]
[null,"5）熟肉制品深加工","吨/班","≥50","50~20","<20"]
[3,"批发、配送与物流仓储工程"]
[null,"1）批发市场工程","万吨/年","≥50","50~20","<20","年交易量"]
[null,"2）棉麻库","万吨","≥3","3~1","<1"]
[null,"3）商业仓库","㎡","≥20000","20000~10000","<10000"]
[null,"4）物资储备仓库","㎡","≥50000","50000~10000","<10000"]
[null,"5）配送中心","㎡","≥30000","30000~10000","<10000"]
[4,"成品油储运工程","万m3","≥10","10~3","<3","总容积"]
[null,null,"万m3","≥2","2~1","<1","单罐容积"]
[5,"粮食工程"]
[null,"1）制粉工程（含玉米加工工程）","原粮吨/日","≥500","500～200","<200"]
[null,"2）碾米工程（及杂粮加工）","原粮吨/日","≥300","300～80","<80"]
[null,"3）饲料加工工程","年单班万吨","≥2","2~1","<1"]
[null,"4）粮食深加工工程","投资万元","≥3000","3000～500","<500"]
[null,"5）粮食仓储工程","仓容万吨","≥15","15～5","<5"]
[5,"5）粮食仓储工程","或投资万元","≥10000","10000～3000","<3000"]
[null,"6）粮油批发交易市场","平方米","≥40000","40000～15000","<15000"]
[6,"油脂工程"]
[null,"1）油脂加工工程","油料吨/日","≥1000","1000～300","<300"]
[null,"2）油脂深加工工程","投资万元","≥3000","3000～500","<500"]
[null,"3）油脂仓储工程","万立方米","≥10","10～4","<4"]

{"sheet":"（九）核工业（1）","index":18,"n_rows":17,"n_cols":28,"rows_kept":17,"merged":[[0,0,0,27],[1,0,2,2],[1,26,2,26],[1,27,2,27],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,12,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,12,1],[13,0,14,0],[13,1,14,1],[15,1,15,27],[16,1,16,27]],"flags":["formulas_cached_only"]}
["（九）核工业行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴核工程与核技术","⑵核安全","⑶机械设备","⑷建筑","⑸结构","⑹电气","⑺暖通","⑻给排水","⑼总图","⑽概预算","⑾自控仪表","⑿环保",{"$nulls":11},"总计","备   注"]
[{"$nulls":3},"核工业","核安全","机械","建筑〔一级〕","结构〔一级〕","电气","公用设备〔暖通空调〕","公用设备〔给水排水〕",null,"造价",null,"环保"]
["行业\n资质","甲级",null,27,2,2,2,4,2,2,2,1,2,2,1,{"$nulls":11},49]
[null,"乙级",{"$nulls":24},0]
["专业\n资质","反应堆工程设计(含核电站总体设计及核岛设计)","甲级",27,2,2,2,4,2,2,2,1,2,2,1,{"$nulls":11},49]
[null,null,"乙级",{"$nulls":23},0]
[null,"核燃料加工制造及处理工程","甲级",25,2,2,2,4,2,2,2,1,2,2,1,{"$nulls":11},47]
[null,null,"乙级",20,1,2,1,2,1,2,1,1,1,1,1,{"$nulls":11},34]
[null,"铀矿山及选冶工程","甲级",15,2,2,2,4,2,4,2,1,1,1,1,{"$nulls":11},37]
[null,null,"乙级",10,1,1,2,2,2,1,1,1,1,1,1,{"$nulls":11},24]
[null,"核设施退役及放射性三废处理处置     工程","甲级",15,2,2,2,4,2,2,1,1,2,2,1,{"$nulls":11},36]
[null,null,"乙级",10,1,2,1,1,1,1,1,1,1,1,1,{"$nulls":11},22]
["专业\n资质","核技术及同位素     应用工程","甲级",5,1,2,1,1,1,1,1,1,1,1,1,{"$nulls":11},17]
[null,null,"乙级",3,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":11},14]
["注：\n","1.  核工程与核技术专业是指：核反应堆工程、核动力工程、核化工、核电子学、核材料、辐射防护、同位素分离、加速器、放射性勘察、铀矿地质、放射性矿产地质等专业。"]
[null,"2.  核工业行业设计资质只设甲级； 核电站及反应堆工程只设甲级。"]

{"sheet":"（九）核工业（2）","index":19,"n_rows":14,"n_cols":8,"rows_kept":14,"merged":[[0,0,0,7],[1,1,1,2],[2,0,3,0],[2,1,3,1],[4,0,8,0],[4,1,8,1],[6,2,7,2],[9,0,11,0],[9,1,11,1],[10,2,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2]],"flags":["formulas_cached_only"]}
["（九）核工业行业建设项目设计规模划分表"]
["序号","建设项目",null,"计量（算）单位","大型","中型","小型","备注"]
[1,"核电及反应堆工程","核电站工程","MWe","≥ 300","300～100","＜  100"]
[null,null,"反应堆工程","亿元","≥ 10","10～1","＜ 1"]
[2,"核燃料加工制造及处理工程","铀转换化工工程","tu/a","≥ 1000","1000～100","＜ 100"]
[null,null,"铀浓缩工程","tSWU /a","≥ 100","100～50","＜ 50"]
[null,null,"燃料元件加工工程","tu/a","≥ 200","200～50","＜ 50"]
[{"$nulls":3},"亿元","≥ 2","2～1","＜ 1"]
[null,null,"乏燃料后处理工程","亿元","≥10","10～5","＜ 5"]
[3,"铀矿山及铀选冶    工程","铀矿山工程","万吨/年","≥ 10","10～5","＜ 5"]
[null,null,"铀选冶工程","万吨/年","≥ 10","10～5","＜ 5"]
[{"$nulls":3},"tu/a","≥ 200","200～100","＜ 100"]
[4,"核设施退役及放射性三废处理处置工程",null,"万元","≥5000","5000～1000","＜ 1000"]
[5,"核技术及同位素应用工程",null,"万元","≥5000","5000～1000","＜ 1000"]

{"sheet":"（十）电子通信广电（1）","index":20,"n_rows":39,"n_cols":41,"rows_kept":39,"merged":[[0,0,0,40],[1,39,2,39],[1,40,2,40],[2,3,2,12],[2,13,2,18],[2,31,2,38],[3,0,8,0],[3,1,4,1],[3,3,3,7],[3,8,3,9],[4,3,4,7],[4,8,4,9],[5,1,6,1],[7,1,8,1],[9,0,16,0],[9,1,10,1],[9,4,9,7],[10,4,10,7],[11,1,12,1],[11,8,11,10],[12,8,12,10],[13,1,14,1],[13,11,13,12],[14,11,14,12],[15,1,16,1],[17,0,30,0],[17,1,18,1],[19,1,20,1],[19,3,19,6],[20,3,20,6],[21,1,22,1],[23,1,24,1],[25,1,26,1],[27,1,28,1],[29,1,30,1],[31,0,36,0],[31,1,32,1],[33,1,34,1],[35,1,36,1],[37,1,37,39],[38,1,38,39]],"flags":["formulas_cached_only"]}
["（十）电子通信广电行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴电子信息工程","⑵雷达及导航","⑶     计算机科学与技术","⑷通信工程","⑸    电子仪器及电子应用产品","⑹电子元件","⑺电子材料","⑻电子机械与结构","⑼显示器件","⑽    集成电路及半导体器件","⑾有线通信","⑿无线通信","⒀电话交换","⒁数据及多媒体","⒂综合布线","⒃邮政及物流机械","⒄自动控制","⒅通信电源","⒆通信铁塔","⒇建筑","(21)结构","(22)规划〔总图〕","(23)动力","(24)暖通","(25)给排水","(26)电气","(27)自控","(28)工程经济","(29)广播电视中心工艺","(30)广播电视发射","(31)广播电视节目传送","(32)电影工艺","(33)声学","(34)塔桅","(35)演播室灯光","(36)天馈线","总计","备   注"]
[{"$nulls":3},"注册工程师（电子）",{"$nulls":9},"注册工程师（通信）",{"$nulls":7},"结构〔一级〕","建筑〔一级〕","结构〔一级〕",null,"公用设备〔动力〕","公用设备〔暖通空调〕","公用设备〔给水排水〕","电气〔供配电〕",null,null,"注册工程师（广电）"]
["行业\n资质","电子工程类","甲级",10,{"$nulls":4},8,null,3,2,6,{"$nulls":9},2,2,1,2,3,2,2,1,2,{"$nulls":8},46]
[null,null,"乙级",5,{"$nulls":4},4,null,2,1,3,{"$nulls":9},1,2,null,1,2,1,1,1,1,{"$nulls":8},25]
[null,"通信工程类","甲级",{"$nulls":10},10,10,10,9,2,3,null,3,3,{"$nulls":17},50]
[null,null,"乙级",{"$nulls":10},6,6,6,5,1,2,null,2,2,{"$nulls":17},30]
[null,"广电工程类","甲级",{"$nulls":19},3,4,null,null,2,1,2,2,2,4,3,3,2,3,3,2,3,39]
[null,null,"乙级",{"$nulls":19},2,2,null,null,2,1,2,1,1,2,2,2,1,2,1,1,1,23]
["专业\n资质","电子整机产品项目工程","甲级",null,12,{"$nulls":17},2,2,null,1,1,1,2,1,2,{"$nulls":8},24]
[null,null,"乙级",null,6,{"$nulls":17},1,1,null,1,1,1,1,1,1,{"$nulls":8},14]
[null,"电子基础产品项目工程","甲级",{"$nulls":5},12,{"$nulls":13},2,2,null,1,1,1,2,1,2,{"$nulls":8},24]
[null,null,"乙级",{"$nulls":5},6,{"$nulls":13},1,1,null,1,1,1,1,1,1,{"$nulls":8},14]
[null,"显示器件  项目工程","甲级",{"$nulls":8},6,{"$nulls":10},2,2,null,1,1,1,2,1,2,{"$nulls":8},18]
[null,null,"乙级",{"$nulls":8},3,{"$nulls":10},1,1,null,1,1,1,1,1,1,{"$nulls":8},11]
[null,"微电子产品项目工程","甲级",{"$nulls":9},6,{"$nulls":9},2,2,null,1,1,1,2,1,2,{"$nulls":8},18]
[null,null,"乙级",{"$nulls":9},3,{"$nulls":10},2,null,1,1,1,1,1,1,{"$nulls":8},11]
["专业\n资质","电子特种环境工程","甲级",6,{"$nulls":19},2,null,1,1,1,2,1,2,{"$nulls":8},16]
[null,null,"乙级",3,{"$nulls":19},1,null,1,1,1,1,1,1,{"$nulls":8},10]
[null,"电子系统    工程","甲级",15,{"$nulls":24},2,1,2,{"$nulls":8},20]
[null,null,"乙级",8,{"$nulls":24},1,1,1,{"$nulls":8},11]
[null,"有线通信","甲级",{"$nulls":10},16,null,10,3,3,null,null,3,{"$nulls":18},35]
[null,null,"乙级",{"$nulls":10},8,null,6,2,2,null,null,2,{"$nulls":18},20]
[null,"无线通信","甲级",{"$nulls":11},18,9,4,{"$nulls":3},4,{"$nulls":18},35]
[null,null,"乙级",{"$nulls":11},10,6,2,{"$nulls":3},2,{"$nulls":18},20]
[null,"邮政工程","甲级",null,null,3,{"$nulls":11},1,9,5,3,{"$nulls":9},1,{"$nulls":8},22]
[null,null,"乙级",null,null,1,{"$nulls":11},1,5,3,1,{"$nulls":9},1,{"$nulls":8},12]
[null,"通信铁塔","甲级",{"$nulls":11},6,6,{"$nulls":5},6,{"$nulls":17},18]
[null,null,"乙级",{"$nulls":11},3,3,{"$nulls":5},3,{"$nulls":17},9]
[null,"广播电视  中心","甲级",{"$nulls":19},3,4,null,null,2,1,2,1,2,4,2,2,null,3,null,2,null,28]
[null,null,"乙级",{"$nulls":19},2,2,null,null,1,1,1,1,1,2,1,1,null,2,null,1,null,16]
["专业\n资质","广播电视  发射","甲级",{"$nulls":19},2,2,null,null,1,1,2,1,2,null,3,2,null,null,3,null,3,22]
[null,null,"乙级",{"$nulls":19},1,1,null,null,1,1,1,1,1,null,2,1,null,null,1,null,2,13]
[null,"广播电视  传输","甲级",{"$nulls":19},2,4,null,null,2,1,2,2,2,1,null,3,{"$nulls":5},19]
[null,null,"乙级",{"$nulls":19},1,1,null,null,1,1,1,1,1,1,1,2,{"$nulls":5},11]
[null,"电影工程","甲级",{"$nulls":19},3,3,null,null,2,2,1,1,2,2,null,1,2,2,null,1,null,22]
[null,null,"乙级",{"$nulls":19},1,2,null,null,1,1,1,1,1,1,null,1,1,1,null,1,null,13]
["注：","1、企业取得电子通信广电行业资质需分别达到电子工程类、通信工程类、广电工程类行业资质标准的要求。"]
[null,"2、注册工程师（电子）、注册工程师（通信）和注册工程师（广电）以国家正式颁布的注册工程师类型划分为准。"]

{"sheet":"（十）电子通信广电（2）","index":21,"n_rows":27,"n_cols":7,"rows_kept":27,"merged":[[0,0,0,6],[16,0,17,0],[16,1,17,1],[18,0,19,0],[18,1,19,1]],"flags":["formulas_cached_only"]}
["（十）电子通信广电行业建设项目设计规模划分表"]
["序号","建设项目","计量\n（算）单位","大型","中型","小型","备注"]
[1,"电子整机产品项目工程","万元","≥10000","10000～3000","＜3000"]
[2,"电子基础产品项目工程","万元","≥10000","10000～3000","＜3000"]
[3,"显示器件项目工程","万元","≥10000","10000～3000","＜3000"]
[4,"微电子产品项目工程","万元","≥10000","10000～3000","＜3000"]
[5,"电子特种环境工程","万元","≥3000\n或国家重点项目","3000～500","＜500"]
[6,"电子系统工程","万元","≥3000\n或国家重点项目","3000～500","＜501"]
[7,"有线通信","万元","≥3000万","＜3000万"]
[8,"无线通信","万元","≥3000万","＜3000万"]
[9,"邮政工程","万元","≥3000万","＜3000万"]
[10,"通信铁塔","万元","≥80米","＜80米"]
[11,"广播中心台","自制节目\n（套数）","≥4","2～3",1]
[12,"电视中心台","自制节目\n（套数）","≥6","3～5","1～2"]
[13,"广播电视中心台","自制节目\n（套数）","≥6","3～5",2]
[14,"中、短波发射台","单机\n发射功率\n（千瓦）","＞150","50～150","≤50"]
[15,"电视、调频发射塔","单机\n发射功率\n（千瓦）","＞10","1～10","≤1","塔高含桅杆高度"]
[null,null,"塔高（米）","≥200","150～200","≤150"]
[16,"有线广播电视网络工程","干线网\n级别","国家、省级","地、市级","县、镇"]
[null,null,"分配网\n用户终端（户）","≥50000","10000～50000","＜1000"]
[17,"微波站","传播方向\n（个）","＞10","4～10","≤4"]
[18,"卫星地球站（下行）","天线直径\n（米）","11～18","5～7","3.7～5"]
[19,"传输网络及网管中心","投资额\n（万元）","＞5000","1000～5000","＜1000"]
[20,"电影制片厂","投资额\n（万元）","＞10000","5000～10000","＜5000"]
[21,"特种电影","所容电影\n系统（注）","70毫米\n（15P或8P）\n巨幕电影","环幕或70毫米立体声电影","70毫米\n（5P）或35毫米环幕电影"]
[22,"立体声影院","所容主要\n电影系统","70毫米宽幕立体声电影","35毫米立体声电影","70毫米非立体声电影 "]
["注：","15P、8P、5P分别表示该电影拷贝上，每一画格所占齿孔数为15个、8个、5个。 "]

{"sheet":"（十一）轻纺（1）","index":22,"n_rows":36,"n_cols":40,"rows_kept":36,"merged":[[0,0,0,39],[1,0,2,2],[1,38,2,38],[1,39,2,39],[2,16,2,18],[3,0,6,0],[3,1,4,1],[3,39,4,39],[5,1,6,1],[5,14,5,15],[5,16,5,18],[5,23,5,25],[6,14,6,15],[6,16,6,18],[6,23,6,25],[7,0,16,0],[7,1,8,1],[7,39,8,39],[9,1,10,1],[9,39,10,39],[11,1,12,1],[11,39,12,39],[13,1,14,1],[13,39,14,39],[15,1,16,1],[15,39,16,39],[17,0,30,0],[17,1,18,1],[17,39,18,39],[19,1,20,1],[19,39,20,39],[21,1,22,1],[21,39,22,39],[23,1,24,1],[23,14,23,15],[23,23,23,25],[24,14,24,15],[24,23,24,25],[25,1,26,1],[25,14,25,15],[25,16,25,18],[25,23,25,25],[26,14,26,15],[26,16,26,18],[26,23,26,25],[27,1,28,1],[27,14,27,15],[27,16,27,18],[27,23,27,25],[28,14,28,15],[28,16,28,18],[28,23,28,25],[29,1,30,1],[29,14,29,15],[29,16,29,18],[29,23,29,25],[30,14,30,15],[30,16,30,18],[30,23,30,25],[31,0,32,0],[31,1,32,1],[31,14,31,15],[31,16,31,18],[31,23,31,25],[32,14,32,15],[32,16,32,18],[32,23,32,25],[33,1,33,39],[34,1,34,39],[35,1,35,39],[36,1,36,39]],"flags":["formulas_cached_only"]}
["（十一）轻纺行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴轻工工艺专业","⑵轻化工专业","⑶设备专业","⑷制浆造纸专业","⑸食品发酵烟草专业","⑹制糖工艺专业","⑺日用化工及塑料专业","⑻日用硅酸盐专业","⑼制盐及盐化工专业","⑽制革专业","⑾轻工机械工艺专业","⑿纺织工艺","⒀服装工艺","⒁染整工艺","⒂化纤原料工艺","⒃化纤工艺","⒄机械　设备","⒅建筑","⒆结构","⒇总图","(21)给排水","(22)暖通","(23)动力","(24)电气","(25)自动控制","(26)环保","(27)技术经济","(28)概预算",{"$nulls":7},"总计","备   注"]
[{"$nulls":4},"化工","机械",{"$nulls":10},"化工",null,null,"机械","建筑〔一级〕","结构〔一级〕",null,"公用设备〔给排水〕","公用设备〔暖通〕","公用设备〔动力〕","电气"]
["\n行业       资质","轻工工程类","甲级",12,5,2,{"$nulls":14},2,4,2,2,2,2,2,2,1,1,1,{"$nulls":7},40,"全行业资质要求：轻工、纺织工艺应覆盖5个专业，每个专业的工艺人员应最少2人。"]
[null,null,"乙级",10,3,1,{"$nulls":14},1,3,1,1,1,1,1,1,1,1,1,{"$nulls":7},27]
[null,"纺织工程类","甲级",{"$nulls":11},4,null,2,null,null,2,2,3,2,2,null,null,2,1,1,1,1,{"$nulls":7},23]
[null,null,"乙级",{"$nulls":11},2,null,1,null,null,1,1,2,1,1,null,null,1,1,1,1,1,{"$nulls":7},14]
["专业\n资质","制浆造纸工程","甲级",null,4,2,4,{"$nulls":13},1,3,1,2,1,2,2,2,1,1,1,{"$nulls":7},27]
[null,null,"乙级",null,2,1,3,{"$nulls":13},1,2,1,1,1,1,1,1,1,1,1,{"$nulls":7},18]
[null,"食品发酵烟草工程","甲级",null,4,2,null,4,{"$nulls":12},1,3,1,2,1,1,2,2,1,1,1,{"$nulls":7},26]
[null,null,"乙级",null,2,1,null,2,{"$nulls":12},1,2,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
[null,"制糖工程","甲级",null,4,2,null,null,4,{"$nulls":11},1,3,1,2,1,2,2,2,1,1,1,{"$nulls":7},27]
[null,null,"乙级",null,2,1,null,null,2,{"$nulls":11},1,2,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
[null,"日化及塑料工程","甲级",null,4,2,{"$nulls":3},4,{"$nulls":10},1,3,1,2,1,1,2,2,1,1,1,{"$nulls":7},26]
[null,null,"乙级",null,2,1,{"$nulls":3},3,{"$nulls":10},1,2,1,1,1,1,1,1,1,1,1,{"$nulls":7},18]
[null,"日用硅酸盐工程","甲级",null,2,1,{"$nulls":4},3,{"$nulls":9},1,3,1,2,1,1,2,2,1,1,1,{"$nulls":7},22]
[null,null,"乙级",null,2,1,{"$nulls":4},2,{"$nulls":9},1,2,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
["专业\n资质","制盐及盐化工程","甲级",null,2,1,{"$nulls":5},3,{"$nulls":8},1,3,1,2,1,1,2,2,1,1,1,{"$nulls":7},22]
[null,null,"乙级",null,2,1,{"$nulls":5},2,{"$nulls":8},1,2,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
[null,"皮革毛皮及制品","甲级",null,2,1,{"$nulls":6},3,{"$nulls":7},1,2,1,2,1,1,2,1,1,1,1,{"$nulls":7},20]
[null,null,"乙级",null,2,1,{"$nulls":6},2,{"$nulls":7},1,2,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
[null,"家电及日用机械","甲级",null,1,2,{"$nulls":7},2,{"$nulls":6},1,2,1,1,1,1,2,1,1,1,1,{"$nulls":7},18]
[null,null,"乙级",null,1,1,{"$nulls":7},1,{"$nulls":6},1,2,1,1,1,1,1,1,1,1,1,{"$nulls":7},15]
[null,"纺织工程","甲级",{"$nulls":11},3,{"$nulls":4},2,1,2,1,2,null,null,2,1,1,1,1,{"$nulls":7},17]
[null,null,"乙级",{"$nulls":11},2,{"$nulls":4},1,1,1,1,1,null,null,1,1,1,1,1,{"$nulls":7},12]
[null,"印染工程","甲级",{"$nulls":13},2,null,null,2,1,2,1,2,null,null,2,1,1,1,1,{"$nulls":7},16]
[null,null,"乙级",{"$nulls":13},1,null,null,1,1,1,1,1,null,null,1,1,1,1,1,{"$nulls":7},11]
[null,"服装工程","甲级",{"$nulls":11},3,{"$nulls":4},2,1,2,1,2,null,null,2,1,1,1,1,{"$nulls":7},17]
[null,null,"乙级",{"$nulls":11},2,{"$nulls":4},1,1,1,1,1,null,null,1,1,1,1,1,{"$nulls":7},12]
[null,"化纤原料工程","甲级",{"$nulls":13},2,null,null,2,1,2,1,2,null,null,2,1,1,1,1,{"$nulls":7},16]
[null,null,"乙级",{"$nulls":13},1,null,null,1,1,1,1,1,null,null,1,1,1,1,1,{"$nulls":7},11]
["专业\n资质","化纤工程","甲级",{"$nulls":13},2,null,null,2,1,2,1,2,null,null,2,1,1,1,1,{"$nulls":7},16]
[null,null,"乙级",{"$nulls":13},1,null,null,1,1,1,1,1,null,null,1,1,1,1,1,{"$nulls":7},11]
[null,"1、表中轻工、纺织工艺专业人员的专业名称如称谓有变革，请参照对应的新学科专业设置。"]
["注：","1、表中轻工、纺织工艺专业人员的专业名称如称谓有变化，请参照对应的新学科专业设置。"]
[null,"2、轻纺工程设计资质，应满足轻工、纺织专业资质中不少于五个专业（1-17）工艺人员的要求；公用专业（18-28）人员要求按轻工行业资质相应甲、乙级资质标准认定。  "]

{"sheet":"（十一）轻纺（2）","index":23,"n_rows":58,"n_cols":8,"rows_kept":58,"merged":[[0,0,0,7],[1,1,1,2],[2,0,5,0],[2,1,5,1],[2,7,5,7],[6,0,11,0],[6,1,11,1],[6,7,11,7],[12,0,13,0],[12,1,13,1],[12,7,13,7],[14,0,18,0],[14,1,18,1],[14,7,18,7],[19,0,20,0],[19,1,20,1],[19,7,20,7],[21,0,22,0],[21,1,22,1],[21,7,22,7],[24,0,25,0],[24,1,25,1],[24,7,25,7],[26,0,29,0],[26,1,29,1],[26,7,29,7],[30,0,35,0],[30,1,35,1],[30,7,35,7],[36,1,36,2],[37,1,37,2],[38,0,41,0],[38,1,41,1],[38,7,41,7],[42,0,50,0],[42,1,50,1],[42,7,46,7],[47,7,55,7],[51,0,55,0],[51,1,55,1],[56,1,56,7],[57,1,57,7]],"flags":["formulas_cached_only"]}
["（十一）轻纺行业建设项目设计规模划分表"]
["序号","建设项目",null,"计量（算）单位","大型","中型","小型","备注"]
[1,"制浆造纸工程","纸板类","万吨/年","≥10","5～10",null,"该行业还包括：生活用纸、涂布加工纸、纸制品、特种纸等。"]
[null,null,"印刷文化用纸","万吨/年","≥5","3～5"]
[null,null,"木材制浆","万吨/年","≥10","5～10"]
[null,null,"非木材制浆","万吨/年","≥5","3.4～5"]
[2,"食品发酵烟草工程","啤酒","万吨/年","≥10","5～10",null,"该行业还包括：酿酒、酒精、味精、发酵制品、淀粉及其衍生物、浓缩果汁、脱水果蔬、各种食品加工制造、食品油脂、食品添加剂、罐头等。"]
[null,null,"饮料","万吨/年","≥5","1～5"]
[null,null,"麦芽","万吨/年","≥5","2～5"]
[null,null,"乳品","吨/日处理鲜奶","≥100","40～100"]
[null,null,"有机酸","万吨/年","≥3","1～3"]
[null,null,"卷烟","万箱/年","≥50","30～50"]
[3,"制糖      工程","甘蔗糖","原料吨/日处理","≥3000","1500～3000",null,"该行业还包括：精制糖、颗粒粕等。"]
[null,null,"甜菜糖","原料吨/日处理","≥2000","1500～2000"]
[4,"日用化工工程","烷基苯","万吨/年","≥7","2～7",null,"该行业还包括：化妆品、油墨及助剂、香精香料、骨胶及胶囊、其他新型电池、合成革等。"]
[null,null,"五钠","万吨/年","≥7","2～7"]
[null,null,"洗衣粉(剂)","万吨/年","≥5","2～5"]
[null,null,"电池","亿只/年","≥3","0.8～3"]
[null,null,"塑料制品","万吨/年","≥1","0.5～1"]
[5,"日用硅酸盐          工程","日用玻璃","万吨/年","≥3","1.5～3",null,"该行业还包括：玻璃仪器、工业陶瓷、医用玻璃、电光源及照明器具等。"]
[null,null,"日用陶瓷","万件/年","≥1000","500～1000"]
[6,"制盐及盐化工工程","海、湖盐","万吨/年","≥70","20～70",null,"该行业还包括：湖、矿盐开采。"]
[null,null,"井矿盐","万吨/年","≥30","10～30"]
[7,"皮革毛皮及制品工程","制革","标准万张/年","≥30","20～30",null,"该行业还包括：羽绒制品、革制品、鞋类等。"]
[8,"家电及日用机械工程","电冰箱","万台/年","≥20","10～20",null,"该行业还包括：空调器、家庭及商用厨房设备、轻工机械、日用五金等。"]
[null,null,"洗衣机","万台/年","≥30","10～30"]
[8,"家电及日用机械工程","压缩机","万台/年","≥100","50～100",null,"该行业还包括：空调器、家庭及商用厨房设备、轻工机械、日用五金等。"]
[null,null,"钟表","万只/年","≥100","40～100"]
[null,null,"缝纫机","万架/年","≥50","15～50"]
[null,null,"自行车","万辆/年","≥100","30～100"]
[10,"纺织\n工程","棉纺工程","万锭","≥5","5～3","＜3","纺织工程包括：棉、毛、麻、丝、化学纤维的粗纺、精纺及机织、针织等"]
[null,null,"毛纺工程（精纺）","锭","≥5000","5000～3000","＜3000"]
[null,null,"毛纺工程（粗纺）","锭","≥3000","3000～1000","＜1000"]
[null,null,"麻纺工程","锭","≥5000","5000～3000","＜3000"]
[null,null,"机织工程","台","≥400","400～200","＜200"]
[null,null,"针织工程","万件/年","≥500","500～300","＜300"]
[11,"印染工程",null,"万米/年","≥5000","5000～1500","＜1500"]
[12,"服装工程",null,"万件/年","≥100","100～60","＜60"]
[13,"化纤原料工程","精对苯二甲酸（PTA)","万吨/年","≥25","25～15",null,"化纤原料工程包括各种化纤原料的生产工程。"]
[null,null,"聚酯工程","万吨/年","≥15","＜15"]
[null,null,"浆粕工程","万吨/年","≥5","＜5"]
[null,null,"棉纶切片工程","万吨/年","≥3","3～1","＜1"]
[14,"化纤\n工程","涤纶长丝工程","万吨/年","≥5","5～2","＜2","化纤长丝工程及化纤短丝工程包括各种纤维品种的工业及民用长丝、短丝工程。　　　　　　　　　　　　　　　　　　　　　　　　　　　　　特种纤维指芳纶、碳纤维等新型纤维、功能纤维和高科技产品"]
[null,null,"丙纶长丝工程","万吨/年","≥1.5","1.5～0.75","＜0.75"]
[null,null,"棉纶长丝工程","万吨/年","≥1.5","1.5～0.5","＜0.5"]
[null,null,"粘胶长丝工程","万吨/年","≥0.6","＜0.6"]
[null,null,"醋纤长丝工程","万吨/年","≥1","＜15"]
[null,null,"涤纤长丝工程\n（含固相增粘）","万吨/年","≥1.5","1.5～0.4","＜0.4","化纤长丝工程及化纤短丝工程包括各种纤维品种的工业及民用长丝、短丝工程。　　　　　　　　　　　　　　　　　　　　　　　　　　　　　特种纤维指芳纶、碳纤维等新型纤维、功能纤维和高科技产品"]
[null,null,"棉纶工业丝工程","万吨/年","≥1.5","1.5～0.4","＜0.4"]
[null,null,"涤纶短纤工程","万吨/年","≥5","5～1.5","＜1.5"]
[null,null,"丙纶短纤工程","万吨/年","≥1.5","1.5～1","＜1"]
[14,"化纤\n工程","腈纶短纤工程","万吨/年","≥5","5～1","＜1"]
[null,null,"粘胶短纤工程","万吨/年","≥5","＜5"]
[null,null,"氨纶工程","万吨/年","≥0.3","0.3～0.1","≤0.1"]
[null,null,"无纺布工程","万吨/年","≥1.2","1.2～0.5","≤0.5"]
[null,null,"特种纤维工程","万吨/年","≥0.5","0.5～0.1","≤0.1"]
["注：\n","1、轻工有22个行业分类，未列入的其他类别还包括：包装、装璜、印刷、家具、文教体育用品、金属制品、衡器、玩具、工艺美术品等行业和产品。"]
[null,"2、鉴于轻工产品品种繁多，未列入上表的设计规模可用设计项目固定资产投资额划分：0.8～1.2亿元为中型，≥1.2亿元为大型。"]

{"sheet":"（十二）建材（1）","index":24,"n_rows":15,"n_cols":24,"rows_kept":15,"merged":[[0,0,0,23],[1,0,2,2],[1,6,1,7],[1,22,2,22],[1,23,2,23],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,14,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,12,1],[13,1,14,1]],"flags":["formulas_cached_only"]}
["（十二）建材行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴建材","⑵电气","⑶建筑","⑷结构",null,"⑸暖通 ","⑹给排水","⑺总图","⑻概预算","⑼技术经济","⑽自动控制","⑾环保",{"$nulls":7},"总计","备   注"]
[{"$nulls":3},"材料","电气","建筑〔二级〕","结构〔一级〕","结构〔二级〕","公用设备〔暖通空调〕","公用设备〔给水排水〕"," "," "]
["行业\n资质","甲级",null,16,3,2,3,1,2,2,2,3,2,2,2,{"$nulls":7},40]
[null,"乙级",null,10,2,1,2,1,1,1,1,2,2,2,1,{"$nulls":7},26]
["专业\n资质","水泥","甲级",9,2,2,2,1,1,2,2,2,2,2,1,{"$nulls":7},28]
[null,null,"乙级",6,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
[null,"玻陶耐","甲级",8,2,2,2,1,1,2,2,2,2,2,1,{"$nulls":7},27]
[null,null,"乙级",6,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
[null,"新材","甲级",8,2,2,2,1,1,2,2,2,2,2,1,{"$nulls":7},27]
[null,null,"乙级",6,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
[null,"非矿","甲级",8,2,2,2,1,1,2,2,2,2,2,1,{"$nulls":7},27]
[null,null,"乙级",6,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]
[null,"无机非金属","甲级",8,2,2,2,1,1,2,2,2,2,2,1,{"$nulls":7},27]
[null,null,"乙级",6,1,1,1,1,1,1,1,1,1,1,1,{"$nulls":7},17]

{"sheet":"（十二）建材（2）","index":25,"n_rows":32,"n_cols":8,"rows_kept":32,"merged":[[0,0,0,7],[1,1,1,2],[2,0,3,0],[2,1,3,1],[4,0,9,0],[4,1,9,1],[10,0,20,0],[10,1,20,1],[21,0,26,0],[21,1,26,1],[23,2,24,2],[23,3,24,3],[27,0,28,0],[27,1,28,1],[29,0,31,0],[29,1,31,1]],"flags":["formulas_cached_only"]}
["（十二）建材行业建设项目设计规模划分表"]
["序号","建设项目",null,"计量（算）单位","大型","中型","小型","备注"]
[1,"水泥厂\n工程","水泥熟料","吨/日","≥3000","﹤3000-2000","﹤2000"]
[null,null,"特种水泥","万吨/年","≥20","﹤20-10","﹤10"]
[2,"玻璃、陶瓷耐火材料          工程","浮法玻璃","吨/日","≥500","﹤500-400","﹤400"]
[null,null,"加工玻璃","万元","≥6000","﹤6000-3000","﹤3000"]
[null,null,"卫生陶瓷","万件/年","≥60","﹤60-30","﹤30"]
[null,null,"建筑陶瓷","万平方米/年","≥150","﹤150-70","﹤70"]
[null,null,"电熔耐火材料","吨/年","≥3000","﹤3000-1500","﹤1500"]
[null,null,"烧结及其它\n耐火材料","吨/年","≥50000","50000-15000","﹤15000"]
[3,"新型建筑\n材料工程","色釉料","万元","≥5000","﹤5000-3000","﹤3000"]
[null,null,"玻璃棉","吨/年","≥6000","﹤6000-2000","﹤2000"]
[null,null,"矿（岩）棉","吨/年","≥10000","﹤10000--5000","﹤5000"]
[null,null,"墙体砖","万块/年","≥6000","﹤6000-3000","﹤3000"]
[null,null,"屋面瓦","万块/年","≥600","﹤600-200","﹤200"]
[null,null,"建筑轻质板材及石膏制品","万元","≥6000","﹤6000-3000","﹤3000"]
[null,null,"保温隔热材料","万元","≥6000","﹤6000-3000","﹤3000"]
[null,null,"装饰装修材料及配套产品","万元","≥6000","﹤6000-3000","﹤3000"]
[null,null,"防水材料及化学建材","万元","≥6000","﹤6000-3000","﹤3000"]
[null,null,"水泥制品及砼砌决等","万元","≥6000","﹤6000-3000","﹤3000"]
[null,null,"商品砼搅拌站","万元","≥6000","﹤6000-3000","﹤3000"]
[4,"非金属\n矿工程","石灰石矿","万吨/年","≥120","﹤120-80","﹤80"]
[null,null,"砂岩矿","万吨/年","≥20","﹤20-5","﹤5"]
[null,null,"石膏矿","万吨/年","≥40","﹤40-20","﹤20","露天"]
[{"$nulls":4},"≥20","﹤20-5","﹤5","地下"]
[null,null,"石墨矿","万吨/年","≥1","﹤1-0.5","﹤0.5"]
[null,null,"石棉矿","万吨/年","≥2","﹤2-0.75","﹤0.75"]
[4,"非金属\n矿工程","石材矿","万平方米/年","≥1","﹤1-0.5","﹤0.5"]
[null,null,"其他非金属矿","万元","≥3000","﹤3000-1000","﹤1000"]
[5,"无机\n非金属材料","玻璃纤维","吨/年","﹥7500","﹤7500-3000","﹤3000"]
[null,null,"玻璃钢","吨/年","≥7500","﹤7500-5000","﹤5000"]
[null,null,"工晶体","万元","≥2000","﹤2000-1000","﹤1000"]

{"sheet":"（十三）铁道（1）","index":26,"n_rows":14,"n_cols":30,"rows_kept":14,"merged":[[0,0,0,29],[1,0,2,2],[1,28,2,28],[1,29,2,29],[3,0,5,0],[3,1,3,2],[4,1,4,2],[5,1,5,2],[6,0,10,0],[11,1,11,29],[12,1,12,29],[13,1,13,29]],"flags":["formulas_cached_only"]}
["（十三）铁道行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴经济","⑵行车","⑶线路","⑷路基","⑸桥梁","⑹隧道","⑺站场","⑻机务","⑼车辆","⑽电气化","⑾信号","⑿通信","⒀建筑","⒁结构","⒂电力","⒃设备","⒄给排水","⒅地质","⒆施工组织","⒇工程经济",{"$nulls":5},"总计","备   注"]
[{"$nulls":5},"土木〔铁路〕","土木〔铁路〕","土木〔结构〕","土木〔铁路〕","土木〔铁路〕",{"$nulls":5},"建筑","结构","电气","机械","公用设备〔给水排水〕 ","岩土",null,"造价"]
["行业\n资质","甲（I）级",null,5,5,10,10,10,10,10,6,6,10,10,6,5,8,8,null,6,10,8,8,{"$nulls":5},151]
[null,"甲（II）级",null,3,3,5,5,5,3,5,3,3,4,4,3,3,3,4,null,3,4,4,4,{"$nulls":5},71]
[null,"乙级",null,1,1,2,2,2,1,2,1,1,2,2,2,1,1,2,null,1,2,2,2,{"$nulls":5},30]
["专业\n资质","桥梁","甲级",null,null,2,2,10,null,1,{"$nulls":5},1,2,1,null,2,6,4,4,{"$nulls":5},35]
[null,"无碴\n轨道","甲级",null,null,2,6,2,2,{"$nulls":4},2,null,null,8,{"$nulls":3},2,2,2,{"$nulls":5},28]
[null,"隧道","甲级",null,null,2,2,null,10,1,{"$nulls":5},1,2,1,2,2,6,4,4,{"$nulls":5},37]
[null,"电气化","甲级",null,null,2,2,null,null,2,null,null,10,null,null,1,1,5,null,null,2,4,4,{"$nulls":5},33]
[null,"通信\n信号","甲级",null,null,1,{"$nulls":7},8,6,1,2,4,null,null,1,4,4,{"$nulls":5},31]
["注：\n","1、甲（I）级设计资质，专业配备的主要专业技术人员均为主持过两项以上特大型项目的专业技术人员。"]
[null,"2、甲（II）级设计资质的主要专业技术人员为主持过两项大型项目的技术人员。"]
[null,"3、乙级设计资质的主要专业技术人员为主持过两项以上中型项目的技术人员。"]

{"sheet":"（十三）铁道（2）","index":27,"n_rows":25,"n_cols":8,"rows_kept":25,"merged":[[0,0,0,7],[21,1,21,7],[22,1,22,7],[23,1,23,7],[24,1,24,7]],"flags":["formulas_cached_only"]}
["（十三）铁道行业建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","特大型","大型","中型","小型","备注"]
[1,"新建铁路","公里","普通铁路≥100，客运专线","100～50","50～10","≤10"]
[2,"改建铁路","公里","普通铁路≥200，客运专线","200～100","100～20","≤20"]
[3,"枢纽","个","各种枢纽","区段站"]
[4,"桥梁","座","深水独立特大桥","特大桥"]
[5,"隧道","座","长度大于5公里","大于2公里"]
[6,"电气化","公里","≥400"]
[7,"通信信号","公里","≥400"]
{"$rows_empty":12}
["注：","1、甲（Ⅰ）级设计单位承担铁路设计任务不受限制。"]
[null,"2、甲（Ⅱ）级设计单位可承担160公里（含）以下的铁路勘察设计，不含200公里以上的山区长大干线和铁路枢纽。"]
[null,"3、铁路行业乙级设计单位可承担时速160公里以下、长度50公里以下的新建铁路和100公里以下既有铁路（不含区段站、特大桥）的勘察设计。"]
[null,"4、铁路专业设计单位承担专业工程涉及的范围不受限制。"]

{"sheet":"（十四）公路（1）","index":28,"n_rows":13,"n_cols":27,"rows_kept":13,"merged":[[0,0,0,26],[1,0,2,2],[1,25,2,25],[1,26,2,26],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,11,0],[5,1,7,1],[10,1,11,1],[12,1,12,26]],"flags":["formulas_cached_only"]}
["（十四）公路行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴路线","⑵路基","⑶路面","⑷互通立交","⑸桥梁","⑹隧道","⑺交通安全设施","⑻    公路工程经济公路工程概算","⑼    公路工程地质水文","⑽环境保护","⑾    系统工程收费系统设备","⑿公路信息传输","⒀    供电照明自控设备","⒁动力","⒂建筑","⒃结构","⒄暖通通风","⒅给排水",{"$nulls":4},"总计","备   注"]
[{"$nulls":17},"建筑〔二级〕","结构〔二级〕"]
["行业\n资质","甲级",null,2,2,2,2,5,5,2,2,2,1,3,2,2,1,1,1,1,1,{"$nulls":4},37]
[null,"乙级",{"$nulls":23},0]
["专业\n资质","公路","甲级",2,2,2,2,2,2,2,2,2,1,1,1,2,1,{"$nulls":8},24]
[null,null,"乙级",2,1,1,1,1,1,2,1,1,1,{"$nulls":12},12]
[null,null,"丙级",1,1,1,null,1,null,1,1,1,{"$nulls":13},7]
[null,"特大\n桥梁","甲级",1,null,1,1,5,null,1,2,2,1,null,1,1,{"$nulls":9},16]
[null,"特长\n隧道","甲级",1,1,1,null,null,5,1,2,2,1,1,1,2,1,{"$nulls":8},19]
[null,"交通\n工程","甲级",1,null,null,1,null,null,1,1,null,1,3,2,2,null,1,1,1,1,{"$nulls":4},16,0]
[null,null,"乙级",1,{"$nulls":5},1,1,null,null,1,null,1,{"$nulls":3},1,1,{"$nulls":4},7]
["注：","未实行注册职业资格制度或实行未满三年的，可暂要求在满足个人设计业绩的基础上，同时满足六年以上设计工作年限的中级及以上技术职称设计人员。已开展注册执业资格制度三年以上的专业原则上按注册人员数量要求。"]

{"sheet":"（十四）公路（2）","index":29,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[21,1,21,6]],"flags":["formulas_cached_only"]}
["（十四）公路行业建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"公路","公路等级或立交形式","高速公路、一级公路、枢纽型互通式立体交叉及其交通安全设施","二级公路及其交通安全设施","三级、四级公路及其交通安全、管理、养护等设施"]
[2,"特大桥梁","长度或跨径","墩高80米以上或单跨跨径150米以上的桥梁"]
[3,"特长隧道","长度或车道 ","长度大于3000米或横断面3个及以上车道的隧道"]
[4,"交通工程","公路等级","高速公路、一级公路的监控系统、通信系统、收费系统及管理、养护、服务设施","二级公路的收费系统及管理、养护、服务设施"]
{"$rows_empty":15}
["注：","未达到特大桥梁、特大隧道标准的桥梁、隧道工程含在各公路规模中。"]

{"sheet":"（十五）水运（1）","index":30,"n_rows":20,"n_cols":30,"rows_kept":20,"merged":[[0,0,0,29],[1,0,2,2],[1,28,2,28],[1,29,2,29],[3,0,4,0],[3,1,3,2],[3,14,3,16],[4,1,4,2],[4,14,4,16],[5,0,12,0],[5,1,6,1],[5,14,5,16],[6,14,6,16],[7,1,8,1],[7,14,7,16],[8,14,8,16],[9,1,10,1],[9,14,9,16],[10,14,10,16],[11,1,12,1],[13,0,16,0],[13,1,14,1],[15,1,16,1],[17,1,17,28],[20,1,20,29]],"flags":["formulas_cached_only"]}
["（十五）水运行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴总平面","⑵航道工程","⑶工程测量","⑷工程水文","⑸工程地质","⑹结构〔港工〕","⑺结构〔金属〕","⑻装卸机械工艺","⑼建筑","⑽土建结构","⑾  铁路道堆桥梁","⑿给排水","⒀动力","⒁暖通","⒂电力电气","⒃自控","⒄通信","⒅环境工程","⒆航海技术","⒇导助航","(21)技术经济","(22)施工    条件概预算",{"$nulls":3},"总计","备   注"]
[{"$nulls":3},"港口与航道","港口与航道",null,null,"岩土","港口与航道",null,null,"建筑〔二级〕","结构",null,"公用设备〔给水排水〕","公用设备〔动力〕","公用设备〔暖通〕","电气"]
["行业\n资质","甲级",null,4,2,1,2,1,4,1,4,1,2,2,2,null,null,1,1,1,1,1,1,1,3,{"$nulls":3},36]
[null,"乙级",null,2,1,null,1,1,2,1,2,1,1,1,1,null,null,1,1,1,1,1,1,1,2,{"$nulls":3},23]
["专业\n资质","港口\n工程","甲级",3,1,1,2,1,4,null,3,1,2,2,2,null,null,1,1,1,1,null,null,1,3,{"$nulls":3},30]
[null,null,"乙级",1,1,null,1,1,2,null,2,1,1,1,1,null,null,1,1,1,1,null,null,1,2,{"$nulls":3},19]
[null,"修造船厂水工工程","甲级",3,null,null,2,1,4,1,2,1,2,null,2,null,null,1,1,1,1,null,null,1,3,{"$nulls":3},26]
[null,null,"乙级",1,null,null,1,1,3,1,1,1,1,null,1,null,null,1,1,1,1,null,null,1,2,{"$nulls":3},18]
[null,"通航建筑工程","甲级",2,1,1,2,1,4,1,null,1,2,null,2,null,null,1,1,1,1,null,null,1,3,{"$nulls":3},25]
[null,null,"乙级",1,1,null,1,1,2,1,null,1,1,null,1,null,null,1,1,1,1,null,null,1,2,{"$nulls":3},17]
[null,"航道\n工程","甲级",2,4,1,2,1,1,null,null,1,2,{"$nulls":7},1,null,2,1,3,{"$nulls":3},21]
[null,null,"乙级",1,2,1,1,null,1,null,null,1,1,{"$nulls":7},1,null,1,1,2,{"$nulls":3},13]
["专业\n资质","水上交通管制工程","甲级",null,2,{"$nulls":13},1,1,1,3,2,1,3,{"$nulls":3},14]
[null,null,"乙级",null,1,{"$nulls":13},1,1,1,1,1,1,2,{"$nulls":3},9]
[null,"港口装卸工艺","甲级",2,{"$nulls":6},4,{"$nulls":9},1,null,null,1,3,{"$nulls":3},11]
[null,null,"乙级",1,{"$nulls":6},2,{"$nulls":9},1,null,null,1,2,{"$nulls":3},7]
["注：","1. 专业资质中水上交通管制工程、港口装卸工艺对注册建筑师及结构师无要求；"]
[null,"2.乙级行业资质和专业资质工程地质、电力电气专业可配置非注册人员；"]
[null,"3.专业资质中水上交通管制工程包含水上交通管制、水上通信导航系统、航标工程；"]

{"sheet":"（十五）水运（2）","index":31,"n_rows":25,"n_cols":10,"rows_kept":25,"merged":[[0,0,0,9],[1,1,1,4],[2,0,12,0],[2,1,12,1],[2,2,9,2],[2,3,3,3],[4,3,5,3],[6,3,7,3],[8,3,9,3],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,0,15,0],[13,1,15,1],[13,2,13,4],[14,2,14,4],[15,2,15,4],[16,0,17,0],[16,1,17,1],[16,2,16,4],[17,2,17,4],[18,0,20,0],[18,1,20,1],[18,2,18,4],[19,2,19,4],[20,2,20,4],[21,0,23,0],[21,1,23,1],[21,2,21,4],[22,2,22,4],[22,5,23,5],[22,6,23,6],[22,7,23,7],[22,8,23,8],[22,9,23,9],[23,2,23,4],[24,2,24,4]],"flags":["formulas_cached_only"]}
["（十五）水运行业建设项目设计规模划分表"]
["序号","建设项目",{"$nulls":3},"计量（算）单位","大型","中型","小型","备注"]
[1,"港口工程","码头","集装箱","沿海","吨级","≥50000","＜50000"]
[{"$nulls":4},"内河","吨级","≥1000","500~1000"]
[{"$nulls":3},"散货","沿海","吨级","≥30000","5000~30000","＜5000"]
[{"$nulls":4},"内河","吨级","≥1000","500~1000","＜500"]
[{"$nulls":3},"件杂货、滚装、客运等多用途","沿海","吨级","≥10000","3000~10000","＜3000"]
[{"$nulls":4},"内河","吨级","≥1000","500~1000","＜500"]
[{"$nulls":3},"原油","沿海","吨级","≥30000","＜30000"]
[{"$nulls":4},"内河","吨级","≥1000","＜1000"]
[null,null,"化学品、成品油\n、气等危险品",null,null,"吨级","≥1000","＜1000"]
[null,null,"防波堤、导流堤\n、海上人工岛等水上建筑",null,null,"最大水深（米）","≥6","＜6"]
[null,null,"护岸、引堤\n、海墙等建筑防护",null,null,"最大水深（米）","≥5","3~5","＜3"]
[2,"修造船厂\n水工工程","船坞",null,null,"船舶吨位","≥10000","3000~10000","＜3000"]
[null,null,"船台、滑道",null,null,"船体重量（吨）","≥5000","1000~5000","＜1000"]
[null,null,"舾装码头",null,null,"吨级","≥10000","3000~10000","＜3000"]
[3,"通航\n建筑工程","渠化枢纽、船闸",null,null,"通航吨级","≥1000","300~1000","＜300"]
[null,null,"升船机",null,null,"通航吨级","≥300","＜300"]
[4,"航道工程","沿海",null,null,"通航吨级","≥30000","＜30000"]
[null,null,"内河整治",null,null,"通航吨级",1000,"300~1000","＜300"]
[null,null,"疏浚与吹填",null,null,"工程量（万方）","≥200","50~200","＜50"]
[5,"水上交通\n管制工程","航标工程",null,null,"投资（万元）","≥1000","＜1000"]
[null,null,"船舶交通管理系统工程",null,null,"投资（万元）","≥3000","＜3000"]
[null,null,"水上通信导航系统工程"]
[6,"港口装卸工艺","港口装卸工艺",null,null,"港口项目规模","大型港口工程中相应装卸工艺 ","中型港口工程中相应装卸工艺 "]

{"sheet":"（十六）民航（1）","index":32,"n_rows":13,"n_cols":29,"rows_kept":13,"merged":[[0,0,0,28],[1,0,2,2],[1,8,1,9],[1,10,1,11],[1,27,2,27],[1,28,2,28],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,12,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,12,1]],"flags":["formulas_cached_only"]}
["（十六）民航行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴机场总体规划","⑵场道","⑶助航灯光","⑷    通信导航航管气象","⑸供油","⑹建筑",null,"⑺结构",null,"⑻电气","⑼给排水","⑽暖通空调","⑾    电子信息〔航站楼弱电〕","⑿环保","⒀概预算",{"$nulls":9},"总计","备   注"]
[{"$nulls":4},"土木工程〔民航〕",null,null,"石油","建筑〔一级〕",null,"结构〔一级〕",null,"电气","公用设备〔给水排水〕","公用设备〔暖通空调〕",null,null,"造价"]
["行业\n资质","甲级",null,6,10,4,8,3,3,5,3,5,3,3,2,2,2,3,{"$nulls":9},62]
[null,"乙级",null,4,6,2,5,2,2,3,2,3,2,2,1,1,1,2,{"$nulls":9},38]
["专业\n资质","机场总体\n规划工程","甲级",6,6,1,2,1,1,1,1,1,2,2,1,1,1,1,{"$nulls":9},28]
[null,null,"乙级",{"$nulls":24},0]
[null,"场道、目视助航    工程","甲级",2,10,2,{"$nulls":6},1,2,{"$nulls":3},3,{"$nulls":9},20]
[null,null,"乙级",{"$nulls":24},0]
[null,"通信、导航、航管及航站楼弱电工程","甲级",{"$nulls":3},8,null,1,null,1,1,2,1,2,2,null,2,{"$nulls":9},20]
[null,null,"乙级",{"$nulls":24},0]
[null,"供油\n工程","甲级",{"$nulls":4},4,1,1,1,1,2,2,2,1,1,2,{"$nulls":9},18]
[null,null,"乙级",{"$nulls":24},0]

{"sheet":"（十六）民航（2）","index":33,"n_rows":24,"n_cols":7,"rows_kept":24,"merged":[[0,0,0,6],[23,0,26,6]],"flags":["formulas_cached_only"]}
["（十六）民航行业建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"民用机场工程","飞行区指标","4E级以上","4D","4C及以下"]
{"$rows_empty":20}
["备注：4E、4D、4C分别为飞行区指标（或称基准代号）。根据民航行业标准《民用机场飞行区技术标准》规定，飞行区技术指标由有关飞机的性能特性和尺寸两个要素组成。第一个要素为使用该机场飞行区跑道的各类飞机中最长的基准飞行场地长度，分为四个等级，分别用阿拉伯数字“1、2、3、4”表示。第二个要素为使用该机场飞行区跑道的各类飞机中最大翼展或最大主起落架外轮外侧边的距离，分为六个等级，分别用英文字母“A、B、C、D、E、F”表示。字母和数字越大，可理解为使用该机场的最大机型越大。"]

{"sheet":"（十七）市政（1）","index":34,"n_rows":37,"n_cols":28,"rows_kept":37,"merged":[[0,3,0,27],[1,0,2,2],[1,3,1,4],[1,5,1,7],[1,8,1,9],[1,10,1,11],[1,12,1,13],[1,14,1,15],[1,22,1,23],[1,24,1,25],[1,26,2,26],[1,27,2,27],[3,0,4,0],[3,1,3,2],[3,27,4,27],[4,1,4,2],[5,0,13,0],[5,1,7,1],[8,1,10,1],[11,1,13,1],[14,0,24,0],[14,1,16,1],[17,1,19,1],[20,1,21,1],[20,27,21,27],[23,1,24,1],[25,0,30,0],[26,1,28,1],[29,1,30,1],[32,1,32,27],[33,1,33,27],[34,1,34,27],[35,1,35,27],[36,1,36,27]],"flags":["formulas_cached_only"]}
[{"$nulls":3},"（十七）市政行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴结构",null,"⑵建筑",null,null,"⑶暖通",null,"⑷给排水",null,"⑸电气",null,"⑹动力",null,"⑺通信信号","⑻站场","⑼道路","⑽线路","⑾桥梁","⑿园林","⒀环保",null,"⒁概预算",null,"总计","备   注"]
[{"$nulls":3},"结构〔一级〕","结构〔二级〕","建筑〔一级〕","建筑〔二级〕",null,"公用设备〔暖通空调〕",null,"公用设备〔给水排水〕",null,"电气〔供配电〕",null,"公用设备〔动力〕",{"$nulls":6},"景观","环保",null,null,"造价"]
["行业\n资质","甲级",null,6,null,3,null,null,2,null,8,null,4,null,4,null,2,2,6,3,6,null,3,null,3,null,52]
[null,"乙级",null,3,null,2,null,null,1,null,4,null,2,null,2,null,0,0,4,0,4,null,2,null,2,null,26]
["专业\n资质","给水    工程","甲级",6,null,1,null,null,1,null,4,2,3,{"$nulls":11},2,null,19]
[null,null,"乙级",3,null,null,1,null,1,null,2,1,2,{"$nulls":11},2,null,12]
[null,null,"丙级",null,1,{"$nulls":6},2,{"$nulls":12},2,null,5]
[null,"排水    工程","甲级",6,null,1,null,null,1,null,4,4,4,{"$nulls":11},2,null,22]
[null,null,"乙级",3,null,null,1,null,1,null,6,null,2,{"$nulls":11},2,null,15]
[null,null,"丙级",null,1,{"$nulls":6},2,{"$nulls":12},2,null,5]
[null,"城镇燃气工程 ","甲级",1,1,null,1,{"$nulls":5},1,null,2,3,{"$nulls":8},2,null,11]
[null,null,"乙级",null,2,null,1,{"$nulls":5},1,null,1,2,{"$nulls":8},2,null,9]
[null,null,"丙级",null,1,null,null,1,{"$nulls":5},1,null,2,{"$nulls":8},2,null,7,"建筑为非注册人员"]
["专业\n资质","热力    工程","甲级",2,null,null,1,{"$nulls":5},3,null,2,3,{"$nulls":8},3,null,14]
[null,null,"乙级",null,1,null,1,{"$nulls":5},1,null,2,2,{"$nulls":8},2,null,9]
[null,null,"丙级",null,1,null,null,1,{"$nulls":5},1,null,2,{"$nulls":8},2,null,7,"建筑为非注册人员"]
[null,"道路    工程","甲级",{"$nulls":7},2,null,2,{"$nulls":5},6,null,2,{"$nulls":3},2,null,14]
[null,null,"乙级",{"$nulls":7},2,null,2,{"$nulls":5},4,null,2,{"$nulls":3},2,null,12]
[null,null,"丙级",{"$nulls":8},1,null,1,{"$nulls":4},2,{"$nulls":5},2,null,6]
[null,"桥梁    工程","甲级",null,null,1,{"$nulls":4},2,null,2,{"$nulls":5},2,null,6,{"$nulls":3},2,null,15]
[null,null,"乙级",{"$nulls":7},2,null,2,{"$nulls":5},2,null,4,{"$nulls":3},2,null,12]
[null,"城市隧道工程设计","甲级",4,{"$nulls":4},2,null,2,null,2,{"$nulls":5},2,null,6,{"$nulls":3},2,null,20]
[null,"公共交通工程","甲级",4,null,1,{"$nulls":4},2,null,2,{"$nulls":7},2,{"$nulls":3},2,null,13]
[null,null,"乙级",2,null,null,1,{"$nulls":3},2,null,2,{"$nulls":7},2,{"$nulls":3},2,null,11]
["专业\n资质","地铁轻轨工程","甲级",4,null,3,null,null,2,null,2,null,2,{"$nulls":3},2,2,null,3,{"$nulls":5},3,23,"车站单项设计适用建筑设计甲级标准，区间单项适用桥隧甲级。"]
[null,"环境卫生工程","甲级",3,null,1,null,null,1,{"$nulls":3},3,null,3,{"$nulls":7},3,null,2,null,16]
[null,null,"乙级",2,null,1,null,null,1,{"$nulls":3},2,null,2,{"$nulls":7},2,null,2,null,12]
[null,null,"丙级",null,1,null,2,null,null,1,{"$nulls":3},1,null,1,{"$nulls":7},1,2,null,9]
[null,"风景园林工程","甲级",1,null,null,2,null,1,null,1,null,1,{"$nulls":8},4,null,null,2,null,12]
[null,null,"乙级",null,1,null,1,null,1,null,1,null,1,{"$nulls":8},2,null,null,2,null,9]
[]
["注：","1、市政公用行业设甲乙级，地铁轻轨工程、城市隧道工程只设甲级。"]
[null,"2、市政全行业工程设计资质甲级须满足桥梁工程和城市隧道工程工程设计类型的要求同时满足不少于6个专业类型的要求；乙级须满足桥梁工程设计类型的要求同时满足不少于5个专业类型的要求。"]
[null,"3、满足市政行业的全部设计资质的要求，但不满足燃气工程、轨道工程的要求，仍可获得市政行业的全部设计资质，但须注明燃气工程、轨道工程除外。"]
[null,"4、给排水、动力专业非注册人员均为高级工程师。"]
[null,"5、取得市政行业资质或风景园林工程专业资质的企业可承担相应级别及范围的园林景观工程专项设计业务。"]

{"sheet":"（十七）市政（2）","index":35,"n_rows":25,"n_cols":9,"rows_kept":25,"merged":[[0,0,0,8],[1,1,1,3],[2,0,3,0],[2,1,3,1],[2,2,2,3],[3,2,3,3],[4,0,6,0],[4,1,6,1],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,0,9,0],[7,1,9,1],[7,2,7,3],[8,2,8,3],[9,2,9,3],[10,0,12,0],[10,1,12,1],[10,2,10,3],[11,2,11,3],[12,2,12,3],[13,1,13,3],[14,1,14,3],[15,1,15,3],[16,1,16,3],[17,1,17,3],[18,0,23,0],[18,1,23,1],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3],[22,2,22,3],[23,2,23,3],[24,0,26,0],[24,1,26,3],[24,4,26,4],[24,5,26,5],[24,6,26,6],[24,7,26,7],[24,8,26,8]],"flags":["formulas_cached_only"]}
["（十七）市政行业建设项目设计规模划分表"]
["序号","建设项目",null,null,"计量（算）单位","大型","中型","小型","备注"]
[1,"给水工程","净水厂",null,"万立方米/日","≧5.0","﹤5 .0"]
[null,null,"管网",null,"万立方米/日","≧10.0、泵站","﹤10 .0","≦5 .0"]
[2,"排水工程","污水处理厂",null,"万立方米/日","≧2.0","﹤2 .0","\\"]
[null,null,"管网",null,"万立方米/日","≧4.0、泵站","﹤4.0","≦2.0"]
[{"$nulls":4},"MM","≧DN1500、泵站","﹤DN1500","≦DN1000"]
[3,"燃气工程","城市燃气输配系统",null,"万立方米/年","≧15000（高、次高、中、低压）","﹤15000（次高、中、低压）","小区管网及户内管（中、低压）","大型工程包括门站、储备站、调压站、各级压力管网系统的整体项目"]
[null,null,"人工气源厂",null,"万立方米/日 ","≧50","﹤50","\\"]
[null,null,"城市液化石油气储备站",null,"瓶/日罐装能力","≧4000","1000~4000","﹤1000"]
[4,"热力工程","热源厂",null,null,"≧3X58MW热水锅炉或3X75t/h蒸气锅炉                        以供热、制冷为主≦单台25MW的小型热电厂 ","≧3X14MW热水锅炉或3X20t/h蒸气锅炉","\\"]
[null,null,"热网系统",null,"供热管道直径","城市供热一级网DN≧800MM，≧7MN热力站","城市供热一级网DN﹤800MM","城市供热二级网DN≦400MM"]
[null,null,"供热面积",null,"万平米","≧500","150~500","﹤150"]
[5,"道路工程",null,null,"等级","城市快速路、主干道、停车场、全苜蓿叶型、双喇叭型、枢纽型等独立的互通式立体交叉工程","城市次干路、简单立体交叉工程","城市支路","停车场指为公众服务的公共停车设施"]
[6,"桥梁工程",null,null,"M","单跨≧40M或总长﹥100M的桥梁","单跨﹤40M或总长﹤100M的桥梁","\\"]
[7,"城市隧道工程",{"$nulls":3},"城市隧道","\\","\\"]
[8,"公共交通工程",{"$nulls":3},"公共交通道路、公交场站、公交枢纽","简单公交停靠站","\\"]
[9,"地铁轻轨工程",{"$nulls":3},"地铁轻轨工程","\\","\\"]
[10,"环境卫生工程（含固体废弃物处理工程）","生活垃圾焚烧工程（含焚烧发电）",null,"T/D","≧200","<200","\\","注：1、取得固体废弃物甲级资质必须做过以上4种大型项目；2、生活垃圾焚烧发电、危险废弃物处理必须由取得甲级资质且有相关业绩的设计单位承担；3、如果上表中不包含危险废弃物及医疗废物，取得甲级资质必须做过3种大型项目"]
[null,null,"卫生填埋",null,"T/D","≧500","200~500","〈200"]
[null,null,"堆（制）肥工程",null,"T/D","≧300","〈300"]
[null,null,"转运站",null,"T/D","≧400","150~400","〈150"]
[null,null,"危险废弃物处理",null,"万吨/年","危险废弃物处理","\\","\\"]
[null,null,"医疗废弃物",null,"T/D","≧5","〈5","\\"]
[11,"风景园林工程",null,null,"万元","投资≥1000万元，高标准的城市重点道路绿化工程，高标准的风景区、公共建筑环境、企事业单位与居住区的绿化工程，公园、度假村、高尔夫球场、广场、街心花园、园林小品、屋顶花园、室内花园等绿化工程。","投资为100~1000万元，标准较高的道路绿化工程，一般标准的风景区、公共建筑环境、企事业单位与居住区的绿化工程。","投资≤100万元，一般标准的道路绿化工程，片林、风景林等工程。"]

{"sheet":"（十八）海洋（1）","index":36,"n_rows":14,"n_cols":31,"rows_kept":14,"merged":[[0,0,0,30],[1,0,2,2],[1,29,2,29],[1,30,2,30],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,11,0],[5,1,6,1],[7,1,8,1],[9,1,10,1],[12,1,12,30],[13,1,13,30]],"flags":["formulas_cached_only"]}
["（十八）海洋行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴海洋规划","⑵海洋动力","⑶工程地质","⑷工艺","⑸海工程结构","⑹浮体性能","⑺舾装","⑻给排水","⑼环保","⑽电气","⑾海洋三防","⑿专用设备","⒀概预算","⒁总图",{"$nulls":12},"总计","备   注"]
[{"$nulls":3},"海洋","海洋","海洋","海洋","海洋",null,"海洋","公用设备〔给水排水〕","环保","电气〔供配电〕","海洋","海洋"]
["行业\n资质","甲级",null,2,4,4,4,8,2,2,1,1,2,2,3,2,2,{"$nulls":12},39]
[null,"乙级",null,1,2,2,2,4,1,1,1,1,1,1,2,1,1,{"$nulls":12},21]
["专业\n资质","沿岸\n工程","甲级",2,4,4,2,8,null,null,1,3,1,1,null,2,2,{"$nulls":12},30]
[null,null,"乙级",1,2,2,1,4,null,null,1,1,1,1,null,1,1,{"$nulls":12},16]
[null,"离岸\n工程","甲级",null,4,2,2,8,2,3,null,1,2,2,null,2,2,{"$nulls":12},30]
[null,null,"乙级",null,2,1,1,4,1,1,null,1,1,1,null,1,1,{"$nulls":12},15]
[null,"海水\n利用","甲级",{"$nulls":3},8,{"$nulls":3},1,2,2,2,5,2,2,{"$nulls":12},24]
[null,null,"乙级",{"$nulls":3},4,{"$nulls":3},1,1,1,1,2,1,1,{"$nulls":12},12]
[null,"海洋能利用","乙级",null,4,null,2,{"$nulls":5},2,2,null,1,1,{"$nulls":12},12]
["注：\n","1、沿岸工程包括围填海工程、防侵蚀工程、护岸护滩工程、堤坝工程、海洋景观、滨海污水海洋处置工程等；离岸工程包括各式海洋平台、海上人工岛礁、离岸海疆固定标志等；海水利用工程包括海水淡化（含苦咸水）、海水直接利用、海底淡水等；海洋能利用工程包括波浪能、潮汐能、潮流能、海底热能等"]
[null,"2、浮体性能是指浮式离岸构筑物在各种设计海况条件下的浮态及运动状态等。"]

{"sheet":"（十八）海洋（2）","index":37,"n_rows":6,"n_cols":7,"rows_kept":6,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["（十八）海洋行业建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"沿岸工程","万元","≥ 8000","8000～2000","≤2000"]
[2,"离岸\n工程","万元","≥ 5000","5000～2000","≤2000"]
[3,"海水利用工程","万元","≥ 1000","1000～200","≤200"]
[4,"海洋能利用工程","万元","≥ 5000","5000～1000","≤1000"]

{"sheet":"（十九）水利（1）","index":38,"n_rows":28,"n_cols":31,"rows_kept":28,"merged":[[0,1,0,30],[1,0,2,2],[1,3,1,4],[1,5,1,6],[1,7,1,8],[1,9,1,10],[1,11,1,12],[1,14,1,15],[1,16,1,17],[1,29,2,29],[1,30,2,30],[3,0,5,0],[3,1,3,2],[4,1,4,2],[4,14,4,15],[5,1,5,2],[6,0,14,0],[6,1,8,1],[6,14,6,15],[7,14,7,15],[9,1,11,1],[9,14,9,15],[10,14,10,15],[11,10,11,11],[12,1,14,1],[12,14,12,15],[13,14,13,15],[14,10,14,11],[15,0,26,0],[15,1,17,1],[15,14,15,15],[16,14,16,15],[17,10,17,11],[18,1,20,1],[18,14,18,15],[19,14,19,15],[20,10,20,11],[21,1,23,1],[21,14,21,15],[22,14,22,15],[23,10,23,11],[23,14,23,15],[24,1,26,1],[24,14,24,15],[25,14,25,15],[26,14,26,15],[27,1,27,30]],"flags":["formulas_cached_only"]}
[null,"（十九）水利行业工程设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴规划",null,"⑵结构",null,"⑶地质",null,"⑷水土保持",null,"⑸征地移民",null,"⑹环境保护","⑺电气",null,"⑻工程造价",null,"⑼水利机械","⑽采暖通风","⑾建筑","⑿观测",{"$nulls":7},"总计","备   注"]
[{"$nulls":3},"土木〔水利水电〕",null,"土木〔水利水电〕",null,"土木〔水利水电〕",null,"土木〔水利水电〕",null,null,"土木〔水利水电〕",null,"电气〔发输变〕",null,"造价"]
["行业\n资质","甲级",null,6,null,10,null,4,null,2,null,2,null,2,1,2,4,null,2,1,1,1,{"$nulls":7},38]
[null,"乙级",null,4,null,5,null,3,null,1,null,1,null,1,2,null,2,null,1,1,1,1,{"$nulls":7},23]
[null,"丙级",null,null,2,null,3,null,2,null,1,1,null,1,null,1,null,1,1,1,1,1,{"$nulls":7},16]
["专业\n资质","水库\n枢纽","甲级",5,null,8,null,3,null,2,null,2,null,2,3,null,3,null,2,1,1,1,{"$nulls":7},33]
[null,null,"乙级",3,null,4,null,2,null,1,null,1,null,1,2,null,2,null,1,1,1,1,{"$nulls":7},20]
[null,null,"丙级",null,2,null,2,null,1,null,1,1,null,1,null,1,null,1,1,1,1,1,{"$nulls":7},14]
[null,"引调水","甲级",4,null,6,null,3,null,1,null,1,null,2,2,null,3,null,2,1,1,1,{"$nulls":7},27]
[null,null,"乙级",3,null,4,null,2,null,1,null,1,null,1,2,null,2,null,1,1,1,1,{"$nulls":7},20]
[null,null,"丙级",null,2,null,2,null,1,null,1,null,null,1,null,1,null,1,1,1,1,1,{"$nulls":7},13]
[null,"灌溉\n排涝","甲级",4,null,6,null,2,null,1,null,1,null,2,2,null,2,null,2,1,1,1,{"$nulls":7},25]
[null,null,"乙级",3,null,4,null,1,null,1,null,1,null,1,2,null,1,null,1,1,1,1,{"$nulls":7},18]
[null,null,"丙级",null,2,null,2,null,1,null,1,null,null,1,null,1,null,1,1,1,1,1,{"$nulls":7},13]
["专业\n资质","河道\n整治","甲级",4,null,6,null,2,null,1,null,1,null,2,1,null,2,{"$nulls":12},19]
[null,null,"乙级",2,null,4,null,1,null,1,null,1,null,1,1,null,1,{"$nulls":12},12]
[null,null,"丙级",null,1,null,2,null,1,null,1,null,null,1,null,1,null,1,{"$nulls":11},8]
[null,"城市\n防洪","甲级",4,null,6,null,2,null,1,null,1,null,2,1,null,2,null,null,1,{"$nulls":9},20]
[null,null,"乙级",2,null,4,null,1,null,1,null,1,null,1,1,null,1,{"$nulls":12},12]
[null,null,"丙级",null,1,null,2,null,1,null,1,null,null,1,null,1,null,1,{"$nulls":11},8]
[null,"围垦","甲级",3,null,5,null,2,null,1,null,1,null,2,null,null,2,{"$nulls":12},16]
[null,null,"乙级",2,null,3,null,1,null,1,null,1,null,1,null,null,1,{"$nulls":12},10]
[null,null,"丙级",null,1,null,2,null,1,null,1,null,null,1,{"$nulls":3},1,{"$nulls":11},7]
[null,"水土\n保持","甲级",2,null,3,null,2,null,2,null,1,null,2,null,null,1,{"$nulls":12},13]
[null,null,"乙级",1,null,2,null,1,null,2,null,1,null,1,null,null,1,{"$nulls":12},9]
[null,null,"丙级",null,1,null,1,null,1,null,1,1,null,1,{"$nulls":3},1,{"$nulls":11},7]
["注：\n","1、申请行业资质甲级或水库枢纽专业资质甲级，电气专业至少需配备1名注册电气工程师（发输变电），其他资质类别电气专业对注册人员不做要求。"]

{"sheet":"（十九）水利（2）","index":39,"n_rows":10,"n_cols":7,"rows_kept":10,"merged":[[0,0,0,6],[2,0,3,0],[2,1,3,1]],"flags":["formulas_cached_only"]}
["（十九）水利行业建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"水库\n枢纽","亿立方米","≥1","1～0.1","＜0.1","库容"]
[null,null,"MW ","≥300","300～50","＜50","装机"]
[2,"引调水","堤防等级","1级","2、3级","4、5级"]
[3,"灌溉\n排涝","立方米/秒","≥5","5～0.5","＜0.5","流量"]
[4,"河道\n整治","万亩","≥30","30～3","＜3","面积"]
[5,"城市\n防洪","万人","≥50","50～20","＜20","城市人口"]
[6,"围垦","万亩","≥5","5～0.5","＜0.5","面积"]
[7,"水土\n保持","平方公里","≥1000","100～100","＜100","综合治理面积"]

{"sheet":"（二十）农林（1）","index":40,"n_rows":30,"n_cols":26,"rows_kept":30,"merged":[[0,1,0,25],[1,0,3,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,7,2,7],[1,8,2,8],[1,9,2,9],[1,10,2,11],[1,12,2,13],[1,14,2,14],[1,15,2,15],[1,16,2,17],[1,18,2,18],[1,19,2,19],[1,20,2,20],[1,21,2,21],[1,22,2,23],[1,24,3,24],[1,25,3,25],[4,0,7,0],[4,1,5,1],[4,18,4,21],[4,25,5,25],[5,18,5,21],[6,1,7,1],[6,14,6,16],[6,18,6,21],[7,14,7,16],[7,18,7,21],[8,0,11,0],[8,1,9,1],[8,25,13,25],[10,1,11,1],[12,0,21,0],[12,1,13,1],[14,1,15,1],[14,25,17,25],[16,1,17,1],[18,1,19,1],[18,14,18,16],[18,18,18,21],[19,14,19,16],[19,18,19,21],[20,1,21,1],[20,14,20,16],[20,18,20,21],[21,14,21,16],[21,18,21,21],[22,0,28,0],[22,1,24,1],[25,1,26,1],[25,18,25,21],[26,18,26,21],[27,1,28,1],[27,18,27,21],[28,18,28,21],[29,1,31,25]],"flags":["formulas_cached_only"]}
[null,"（二十）农林行业工程设计主要专业技术人员配备表"]
[{"$nulls":3}," 农业工程     （种植、畜牧、兽医、渔港、水文/地质、渔捞、农机、农业建筑、农田水利、资源环境、牧草、农村能源、农畜水产品加工及贮藏、农业废弃物处理、农业综合开发等）","林产工业  （木材加工、人造板、木工机械、建筑材料）","林产化工（各类化工、化工机械、制浆、造纸、缄回收、污水处理）","营林造林（林学、水土保持、土壤、森林经理、规划、森林生态、园林）","环境保护（生物、动物、植物、环境保护、森林保护）","森林工程（森林经营、总图规划、采运、道桥、测量、机械）","农业工程规划","建筑",null,"结构",null,"给排水","暖通空调","电力",null,"自控","通信","热力","燃气","造价",null,"总计","备注"]
[]
[{"$nulls":11},"建筑〔一级、二级〕",null,"结构〔一级、二级〕","公用设备〔给排水〕","公用设备〔暖通〕","公用设备〔电力〕","电 气 ",{"$nulls":5},"造价"]
["行业 资质","农业  工程类","甲级",17,{"$nulls":5},3,"2","⑴","5","⑴","2",2,2,null,"2",{"$nulls":3},"2","1","40","申请农业工程各设计类型，应分别满足对相应类型工艺人员的实际需要"]
[null,null,"乙级",12,{"$nulls":5},1,1,"①",3,"①",1,1,1,null,1,{"$nulls":3},1,null,24]
[null,"林业  工程类","甲级",null,5,4,10,5,2,null,"1","⑴","1","⑴","2",null,null,"2","3",{"$nulls":3},"3",null,"40"]
[null,null,"乙级",null,3,2,5,2,1,null,"1","⑴","1","⑴","2",null,null,"1","2",{"$nulls":3},"2",null,"24"]
["专业   资质","农业综合开发生态 工程","甲级",8,{"$nulls":5},1,1,null,1,null,1,1,1,{"$nulls":5},1,null,15,"        未注册的建筑结构工程师均为从事相关专业技术工作5年（含5年）以上。                     "]
[null,null,"乙级",6,{"$nulls":5},1,null,null,1,{"$nulls":3},1,{"$nulls":5},1,null,10]
[null,"种植业 工程","甲级",8,{"$nulls":5},1,1,null,1,null,1,1,1,{"$nulls":5},1,null,15]
[null,null,"乙级",6,{"$nulls":5},1,null,null,1,null,1,1,1,{"$nulls":5},1,null,12]
["专业   资质","兽医/  畜牧工程","甲级",7,{"$nulls":5},1,1,null,2,null,1,1,1,{"$nulls":5},1,null,15]
[null,null,"乙级",5,{"$nulls":8},1,null,1,1,1,{"$nulls":5},1,null,10]
[null,"渔业  工程","甲级",8,{"$nulls":5},1,null,null,2,null,1,1,1,{"$nulls":5},1,null,15,"同上"]
[null,null,"乙级",5,{"$nulls":8},1,null,1,1,1,{"$nulls":5},1,null,10]
[null,"设施  农业  工程","甲级",7,{"$nulls":5},1,1,null,2,null,1,1,1,{"$nulls":5},1,null,15]
[null,null,"乙级",4,{"$nulls":8},2,null,1,1,1,{"$nulls":5},1,null,10]
[null,"林产  工业  工程","甲级",null,5,2,null,1,1,null,1,"①",2,"①",2,null,null,2,5,{"$nulls":3},1,1,25]
[null,null,"乙级",null,3,1,{"$nulls":4},1,1,1,1,2,null,null,1,2,{"$nulls":3},1,null,14]
[null,"林产  化学  工程","甲级",null,2,4,null,1,1,null,null,"②",null,"②",2,null,null,2,5,{"$nulls":3},1,1,23]
[null,null,"乙级",null,1,2,{"$nulls":4},1,1,1,1,2,null,null,1,2,{"$nulls":3},1,null,13]
["专业   资质","营造林 工程","甲级",{"$nulls":3},16,3,4,{"$nulls":13},1,null,24]
[null,null,"乙级",{"$nulls":3},9,2,1,{"$nulls":13},1,null,13]
[null,null,"丙级",{"$nulls":3},6,{"$nulls":15},1,null,7]
[null,"森林资源环境工程","甲级",{"$nulls":3},10,8,{"$nulls":4},2,{"$nulls":5},2,{"$nulls":3},2,null,24]
[null,null,"乙级",{"$nulls":3},3,6,{"$nulls":4},1,{"$nulls":5},1,{"$nulls":3},1,null,12]
[null,"森林  工业  工程","甲级",{"$nulls":3},9,3,7,{"$nulls":3},2,{"$nulls":5},2,{"$nulls":3},2,null,25]
[null,null,"乙级",{"$nulls":3},4,1,5,{"$nulls":3},1,{"$nulls":5},1,{"$nulls":3},1,null,13]
["备注：","1、申请农林全行业资质，应满足农业、林业各3个设计类型甲级或乙级要求，为农林全行业甲级或乙级；                                                                                                                            2、申请农业行业资质，应满足3个以上农业设计类型甲级或乙级要求，为农林行业（农业工程）甲级或乙级；                                                                                                    3、申请林业行业资质，应满足3个以上林业设计类型甲级或乙级要求，为农林行业（林业工程）甲级或乙级；                                                                                                                          4、满足某项设计类型，可具有单项资质，如：农林行业（渔业工程）甲级，农林行业（林产工业、林产化工）乙级。                                                                                                                                                                                                                                                                                                                                              5、（）内的数字为一级注册建筑师或一级注册结构工程师；○内数字为二级注册建筑师或二级注册结构工程师。                                       "]

{"sheet":"（二十）农林（2）","index":41,"n_rows":106,"n_cols":7,"rows_kept":106,"merged":[[0,0,0,6],[1,4,1,5],[2,1,2,6],[3,4,3,5],[4,4,4,5],[5,4,5,5],[6,4,6,5],[7,4,7,5],[8,4,8,5],[9,4,9,5],[10,4,10,5],[11,4,11,5],[12,1,12,6],[13,4,13,5],[14,4,14,5],[15,4,15,5],[16,4,16,5],[17,4,17,5],[18,4,18,5],[19,4,19,5],[20,4,20,5],[21,4,21,5],[22,4,22,5],[23,4,23,5],[24,4,24,5],[25,4,25,5],[26,4,26,5],[27,4,27,5],[28,4,28,5],[29,4,29,5],[30,4,30,5],[31,4,31,5],[32,1,32,6],[33,4,33,5],[34,1,34,6],[35,4,35,5],[36,4,36,5],[37,4,37,5],[38,4,38,5],[39,1,39,5],[40,4,40,5],[41,4,41,5],[42,4,42,5],[43,4,43,5],[44,4,44,5],[45,4,45,5],[46,4,46,5],[47,4,47,5],[48,4,48,5],[49,4,49,5],[50,1,50,6],[51,4,51,5],[52,4,52,5],[53,4,53,5],[54,4,54,5],[55,4,55,5],[56,1,56,6],[57,4,57,5],[58,4,58,5],[59,4,59,5],[60,4,60,5],[61,4,61,5],[62,4,62,5],[63,4,63,5],[64,1,64,6],[69,1,69,6],[80,1,80,6],[86,1,86,6]],"flags":["formulas_cached_only"]}
["（二十）农林行业建设项目设计规模划分表"]
["序号","建设项目","计量单位","大型","中小型",null,"备注"]
[1,"种植业工程"]
["(1)","商品粮基地","万亩","≥10","＜10"]
["(2)","商品棉基地","万亩","≥10","＜10"]
["(3)","商品油料基地","万亩","≥2","＜2"]
["(4)","商品糖料基地","万亩","≥2","＜2"]
["(5)","作物种子良繁基地","万亩","≥1","＜1"]
["(6)","果苗基地","万亩","≥0.3","＜0.3"]
["(7)","蔬菜种子良繁基地","万亩","≥1","＜1"]
["(8)","种子库","万吨","≥1","＜1"]
["(9)","橡胶种植基地","万亩","≥4","＜4"]
[2,"兽医/畜牧工程"]
["(1)","种鸡场","万只/存栏","≥2","＜2"]
["(2)","商品肉鸡场","万只/出栏","≥100","＜100"]
["(3)","商品蛋鸡场","万只/存栏","≥20","＜20"]
["(4)","种猪场","头/存栏","≥600","＜600"]
["(5)","商品猪场","万头/出栏","≥3","＜3"]
["(6)","肉牛种牛场","头/存栏","≥800","＜800"]
["(7)","奶牛种牛场","头/存栏","≥1200","＜1200"]
["(8)","肉牛场","万头/存栏","≥1","＜1"]
["(9)","奶牛场","头/存栏成母牛","≥500","＜500"]
["(10)","种羊场","头/基础母羊","≥150","＜150"]
["(11)","商品羊场","头/存栏","≥3000","＜3000"]
["(12)","实验动物房工程","平方米","≥1000","＜1000"]
["(13)","兽医生物制品厂工程","亿头份/年产","≥1","＜1"]
["(14)","兽医二级以上生物实验室","平方米","≥3000","＜3000"]
["(15)","草场建设工程","万亩","≥5","＜5"]
["(16)","饲料加工厂","吨/小时","≥10","＜10"]
["(17)","鸡屠宰厂","只/小时","≥2000","＜2000"]
["(18)","猪屠宰厂","头/小时","≥250","＜250"]
["(19)","牛屠宰厂","头/小时","≥25","＜25"]
[3,"渔业工程"]
["(1)","渔港工程","万元","≥3000","＜3000"]
["(2)","水产养殖工程"]
[null,"海水养殖","亩","≥2000","＜2000"]
[null,"淡水养殖","亩","≥1000","＜1000"]
[null,"网箱养殖","箱","≥6000","＜6000"]
[null,"设施渔业","万元","≥2500","＜2500"]
["(3)","冷藏加工"]
[null,"水产冷库","吨/次","≥5000","＜5000"]
[null,"储冰库","吨/次","≥4000","＜4000"]
[null,"水产品加工","吨/年","≥3000","＜3000"]
[null,"水产饲料加工","吨/年","≥10000","＜10000"]
["(4)","水产批发市场及配发中心","平方米","≥5000","＜5000"]
["(5)","水产原、良种工程","亿尾","≥5","＜5"]
["(6)","人工鱼礁工程","万元","≥3000","＜3000"]
["(7)","渔场建设与修复工程","万元","≥3000","＜3000"]
["(8)","渔业环境与水产动物保护工程","万元","≥1500","＜1500"]
["(9)","鱼病防治工程","万元","≥2000","＜2000"]
[4,"农业综合开发工程"]
["(1)","土地治理工程","万亩","≥5","＜5"]
["(2)","高科技农业园艺工程","万亩","≥1","＜1"]
["(3)","农业废弃物处理工程","吨/日处理","≥150","＜150"]
["(4)","农业生态工程","万亩","≥10","＜10"]
["(5)","可再生能源工程","万元","≥1000","＜1000"]
["5","设施农业工程"]
["(1)","设施园艺工程","公顷","≥1","＜1"]
["(2)","种子加工工程","吨/小时","≥5","＜5"]
["(3)","谷物及粮食加工工程","万吨/年","≥2","＜2"]
["(4)","果蔬加工工程","万吨/年","≥1","＜1"]
["(5)","糟渣及饼粕加工工程","万吨/年","≥0.6","＜0.6"]
["(6)","天然橡胶产品加工工程","万吨/年","≥3","＜3"]
["(7)","饲草加工工程","万吨/年","≥3","＜3"]
["6","林产工业工程"]
["(1)","木材加工（制材）","m3/a","＞200000","200000～100000","＜100000"]
["(2)","人造板加工","m3/a","＞200000","200000～100000","＜100000"]
["(3)","装饰板加工","㎡/a","＞6000000","6000000～1800000","＜1800000"]
["(4)","实木复合板","㎡/a","＞500000","500000～200000","＜200000"]
["7","林产化学工程"]
["(1)","制胶","t/a","＞20000","20000～5000","＜5000","以固体含量100%计"]
["(2)","栲胶","t/a","＞3000","3000～1000","＜1000"]
["(3)","松香","t/a","＞10000","10000～5000","＜5000"]
["(4)","植物纤维水解","t/a","＞3000","3000～1000","＜1000"]
["(5)","木材热解","t/a","＞3000","3000～1000","＜1000"]
["(6)","制浆造纸"]
[null,"木浆","t/a","＞200000","200000～100000","＜100000"]
[null,"竹浆","t/a","＞100000","100000～50000","＜50000"]
[null,"纸浆","t/a","＞150000","150000～80000","＜80000"]
[null,"纸 ","t/a","＞100000","100000～50000","＜50000"]
["8","营林造林工程"]
["(1)","人工造林、飞播造林、营林","hm2","＞10000","1000～10000","＜1000"]
["(2)","封山（沙）育林","hm2","＞20000","20000～2000","＜2000"]
["(3)","种子、苗木及花卉基地","hm2","＞60","60～20","＜20"]
["(4)","国土绿化美化","万元","＞1000","1000～100","＜100"]
["(5)","生态观光园","hm2","＞200","200～100","＜100"]
["9","森林资源环境工程"]
["(1)","自然保护区"]
[null,"森林类型","hm2","50000","50000～10000","10000"]
[null,"湿地类型","hm2","80000","80000～20000","20000"]
[null,"荒漠类型","hm2","200000","200000～50000","50000"]
[null,"野生植物类型","hm2","10000","10000～5000","5000"]
[null,"野生动物类型","hm2","100000","100000～20000","20000"]
[null,"自然遗迹类型","hm2","30000","30000～50000","5000"]
["(2)","森林公园","hm2","＞5000","5000～2000","＜2000"]
["(3)","野生动植物园","hm2","＞200","200～100","＜100"]
["(4)","天然林保护","hm2","＞200000","200000～50000","＜50000"]
["(5)","森林防火","hm2","＞200000","200000～50000","＜50000","控制面积"]
["(6)","病虫害防治","hm2","＞20000","20000～10000","＜10000","防治面积"]
["(7)","湿地资源保护与恢复","hm2","＞10000","10000～5000","＜5000"]
["(8)","野生动植物资源及其栖息地保护与恢复","hm2","＞2000","2000～500","＜500"]
["10","森林工业工程"]
["(1)","贮木场","m3/年","＞150000","150000～50000","＜50000"]
["(2)","林业综合开发","hm2","＞10000","10000～3500","＜3500"]
["(3)","高科技林业示范园","hm2","＞650","650～200","＜200"]
["(4)","林区森林资源开发","hm2","＞350000","350000～150000","＜150000"]

{"sheet":"（二十一）建筑（1）A","index":42,"n_rows":11,"n_cols":26,"rows_kept":11,"merged":[[0,0,0,25],[1,0,2,2],[1,3,1,5],[1,6,1,8],[1,9,1,10],[1,11,1,12],[1,13,1,14],[1,24,2,24],[1,25,2,25],[3,0,4,0],[3,1,3,2],[4,1,4,2],[5,0,9,0],[5,1,7,1],[8,1,9,1],[10,1,10,25],[11,1,11,25]],"flags":["formulas_cached_only"]}
["（二十一）建筑行业工程设计主要专业技术人员配备表（1）"]
[{"$nulls":3},"⑴建筑",null,null,"⑵结构",null,null,"⑶给排水",null,"⑷暖通",null,"⑸电气",null,"⑹防护","⑺防化","⑻通信","⑼核电磁脉冲防护","⑽概预算",{"$nulls":4},"总计","备   注"]
[{"$nulls":3},"建筑〔一级〕","建筑〔二级〕",null,"结构〔一级〕","结构〔二级〕",null,"公用设备〔给水排水〕",null,"公用设备〔暖通空调〕",null,"注册电气师"]
["行业\n资质","甲级",null,3,null,5,3,null,5,2,2,2,2,2,2,3,1,2,1,1,{"$nulls":4},36]
[null,"乙级",null,2,null,4,2,null,4,1,2,1,2,1,2,2,0,1,0,1,{"$nulls":4},25]
["专业\n资质","建筑工程","甲级",3,null,3,3,null,3,1,2,1,2,1,2,{"$nulls":9},21]
[null,null,"乙级",2,null,1,2,null,1,1,1,1,1,1,1,{"$nulls":9},12]
[null,null,"丙级",null,2,null,null,2,null,null,1,null,1,null,1,{"$nulls":9},7]
[null,"人防工程","甲级",1,null,3,2,null,1,null,2,1,1,1,1,3,1,2,1,1,{"$nulls":4},21,"防护专业3人、通信专业1人为高工"]
[null,null,"乙级",null,1,1,null,2,null,null,1,1,null,1,null,2,null,1,null,1,{"$nulls":4},11,"防护专业1人为高工，结构专业可为一名一级注册师或两名二级注册师"]
["注：","1、取得建筑工程设计资质的企业均可承担相应的附建式人防项目。2、核电磁脉冲防护专业人员可由经过必要培训学习后的电气专业人员代替。3、防护专业、通信专业、防化专业人员，均指从事人防工程该专业设计工作并有相应业绩的人员。4、具有建筑工程甲级、乙级资质的企业可以承担相应级别和范围内的建筑装饰、建筑智能化、建筑幕墙、轻型房屋钢结构、园林景观和消防设施工程设计业务。 "]

{"sheet":"（二十一）建筑（1）B","index":43,"n_rows":17,"n_cols":6,"rows_kept":17,"merged":[[0,0,0,5],[2,0,11,0],[2,1,11,1],[5,2,11,2],[12,0,13,0],[12,1,13,1],[15,0,16,0],[15,1,16,1]],"flags":["formulas_cached_only"]}
["（二十一）建筑行业建设项目设计规模划分表"]
["序号","建 设 项 目","工程等级特征","大  型","中 型","小 型"]
[1,"一般公共建筑","单体建筑面积","20000㎡～80000㎡","5000㎡～20000㎡","≤5000㎡"]
[null,null,"立项投资","4000万～20000元","1000万～4000万元","≤1000万元"]
[null,null,"建筑高度","＞50m","24m～50m","≤24m"]
[null,null,"复杂程度","1.高级大型公共建筑工程"," 1.大中型公共建筑工程","1.功能单一、技术要求简单的小型公共建筑工程"]
[{"$nulls":3},"2.技术要求复杂或具有经济、文化、历史等意义的省（市）级中小型公共建筑工程","2.技术要求复杂或有地区性意义的小型公共建筑工程","2.高度＜24m的一般公共建筑工程"]
[{"$nulls":3},"3.高度＞50m的公共建筑工程","3.高度24－50m的一般公共建筑工程","3.小型仓储建筑工程"]
[{"$nulls":3},"4.相当于四、五星级饭店标准的室内装修、特殊声学装修工程","4.仿古建筑、一般标准的古建筑、保护性建筑以及地下建筑工程","4.简单的设备用房及其它配套用房工程"]
[{"$nulls":3},"5.高标准的古建筑、保护性建筑和地下建筑工程","5.大中型仓储建筑工程","5.简单的建筑环境设计及室外工程"]
[{"$nulls":3},"6.高标准的建筑环境设计和室外工程","6.一般标准的建筑环境设计和室外工程","6.相当于一星级饭店及以下标准的室内装修工程"]
[{"$nulls":4},"7.相当于二、三星级饭店标准的室内装修工程"]
[2,"住宅  宿舍","层数","＞20层","12层～20层","≤12层（其中砌块建筑不得超过抗震规范层数限值要求）"]
[null,null,"复杂程度","20层以上居住建筑和20层及以下高标准居住建筑工程","20层及以下一般标准的居住建筑工程"]
[3,"住宅小区工厂生活区","总建筑面积","＞30万㎡规划设计","≤30万㎡规划设计","单体建筑按上述住宅或公共建筑标准执行"]
[4,"地下  工程","地下空间（总建筑面积）","＞1万㎡","≤1万㎡"]
[null,null,"附建式人防（防护等级）","四级及以上","五级及以下","人防疏散干道、支干道及人防连接通道等人防配套工程"]

{"sheet":"（二十一）建筑（2）A","index":44,"n_rows":8,"n_cols":26,"rows_kept":8,"merged":[[0,0,0,25],[1,0,2,2],[1,3,1,5],[1,6,1,8],[1,9,1,10],[1,11,1,12],[1,13,1,14],[1,24,2,24],[1,25,2,25],[3,0,5,0],[6,1,6,25],[7,1,7,25]],"flags":["formulas_cached_only"]}
["（二十一）建筑行业设计事务所主要专业技术人员配备表（2）"]
[{"$nulls":3},"⑴建筑",null,null,"⑵结构",null,null,"⑶给排水",null,"⑷暖通",null,"⑸电气",null,"⑹防护","⑺防化","⑻通信","⑼核电磁脉冲防护","⑽概预算",{"$nulls":4},"总计","备   注"]
[{"$nulls":3},"建筑〔一级〕","建筑〔二级〕",null,"结构〔一级〕","结构〔二级〕",null,"公用设备〔给水排水〕",null,"公用设备〔暖通空调〕",null,"注册电气师"]
["事务所    资质","建筑专业","甲级",3,{"$nulls":20},3]
[null,"结构专业","甲级",{"$nulls":3},3,{"$nulls":17},3]
[null,"机电专业","甲级",{"$nulls":6},2,null,2,null,2,{"$nulls":10},6,"相关专业注册人员二人（机电与电气专业合为机电专业）"]
["注：","1、建筑专业 / 结构专业事务所可以承接所有建筑工程等级的项目方案设计、初步设计及施工图设计中的建筑专业 / 结构专业(包括轻钢结构)设计与咨询业务。"]
[null,"2、机电设计事务所可以承揽建筑工程（包括建筑智能化设计）方案设计、初步设计及施工图设计中的机电设备专业的设计与咨询业务。"]

{"sheet":"（二十一）建筑（2）B","index":45,"n_rows":7,"n_cols":7,"rows_kept":7,"merged":[[0,0,0,6],[2,6,6,6],[3,3,6,3],[3,4,6,4],[3,5,6,5]],"flags":["formulas_cached_only"]}
["（二十一）建筑行业设计事务所建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"人防指挥工程","万元","＞1000（含）","＜1000",null,"各级人防\n指挥工程"]
[2,"医疗救护工程","万元","＞2000（含）","600（含）\n～2000","200（含）\n～600"]
[3,"防空专业队工程","万元"]
[4,"人员掩蔽工程","万元"]
[5,"人防配套工程","万元"]

{"sheet":"（1）建筑装饰A","index":46,"n_rows":6,"n_cols":31,"rows_kept":6,"merged":[[0,0,0,30],[1,0,2,2],[1,29,2,29],[1,30,2,30],[3,0,5,0],[3,1,5,1],[3,3,3,5],[4,3,4,5],[5,3,5,5]],"flags":["formulas_cached_only"]}
["（1）建筑装饰工程专项设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴环境艺术设计","⑵室内设计","⑶建筑","⑷电气","⑸给排水","⑹暖通","⑺空调","⑻结构",{"$nulls":18},"总计","备   注"]
[]
["专项\n资质","建筑装饰工程","甲级",5,null,null,1,1,1,1,1,{"$nulls":18},10]
[null,null,"乙级",3,null,null,1,1,1,{"$nulls":20},6]
[null,null,"丙级   （家装）",2,null,null,1,1,{"$nulls":21},4]

{"sheet":"（1）建筑装饰B","index":47,"n_rows":3,"n_cols":7,"rows_kept":3,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["（1）建筑装饰工程建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"建筑装饰工程","万元人民币","≥1000万元","500～1000万元","＜500万元"]

{"sheet":"（2）建筑智能化A","index":48,"n_rows":6,"n_cols":30,"rows_kept":6,"merged":[[0,0,0,29],[1,0,2,2],[1,28,2,28],[1,29,2,29],[3,0,4,0],[3,1,4,1],[5,1,5,29],[6,1,6,29]],"flags":["formulas_cached_only"]}
["（2）建筑智能化系统集成专项设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴自动化","⑵通信信息","⑶计算机","⑷机电一体化","⑸给排水","⑹暖通空调","⑺机械","⑻环保",{"$nulls":17},"总计","备   注"]
[{"$nulls":3},"电气自控","电子                〔电子信息、广播电影电视〕"]
["专项\n资质","建筑智能化系统集成设计","甲级",4,3,3,4,1,2,2,1,{"$nulls":17},20]
[null,null,"乙级",2,1,1,1,1,1,1,{"$nulls":18},8]
["注： ","1、专业设置中，自动化包括自控、电子、仪表；计算机包括网络、软件工程、电子；通信包括有线通信、无线通信、卫星通信、微波、广播电视，机电安装包括机械、公用设备、电气；"]

{"sheet":"（2）建筑智能化B","index":49,"n_rows":3,"n_cols":7,"rows_kept":3,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["（2）建筑智能化系统集成建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"建筑智能化系统集成设计项目","万元人民币","＞1000或国家重点项目","500～1000","＜500"]

{"sheet":"（3）建筑幕墙A","index":50,"n_rows":5,"n_cols":31,"rows_kept":5,"merged":[[0,0,0,30],[1,0,2,2],[1,29,2,29],[1,30,2,30],[3,0,4,0],[3,1,4,1],[3,3,3,4],[4,3,4,4]],"flags":["formulas_cached_only"]}
["（3）建筑幕墙工程专项设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴建筑","⑵结构","⑶机械",{"$nulls":23},"总计","备   注"]
[]
["专项\n资质","建筑幕墙工程","甲级",4,null,6,{"$nulls":23},10,"其中有一名是高级技术职称或一级职业注册资格"]
[null,null,"乙级",2,null,3,{"$nulls":23},5,"其中有一名是高级技术职称或一级职业注册资格"]

{"sheet":"（3）建筑幕墙B","index":51,"n_rows":3,"n_cols":7,"rows_kept":3,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["（3）建筑幕墙工程建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"建筑幕墙工程","平方米","工程面积           ≥6000m2","工程面积2000m2 ～6000m2","工程面积        ＜2000m2"]

{"sheet":"（4）钢结构A","index":52,"n_rows":8,"n_cols":31,"rows_kept":8,"merged":[[0,0,0,30],[1,0,2,2],[1,4,1,6],[1,29,2,29],[1,30,2,30],[3,0,6,0],[3,1,6,1],[7,0,7,30]],"flags":["formulas_cached_only"]}
["（4）轻型房屋钢结构工程专项设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴建筑","⑵结构",null,null,"⑷焊接","⑸技术经济","⑹其他",{"$nulls":19},"总计","备   注"]
[{"$nulls":3},"建筑〔二级〕","结构〔一级〕","结构〔二级〕",null,"机械  ","造价"]
["专项\n资质","轻型房屋钢结构工程","甲级",1,2,null,3,1,1,{"$nulls":20},8]
[null,null,"乙级",null,1,null,2,1,1,{"$nulls":20},5]
[null,null,"索膜结构",null,null,1,1,1,1,{"$nulls":20},4]
[null,null,"压型拱板",null,null,1,1,1,1,{"$nulls":20},4]
["                  注：取得索膜结构和压型拱板设计资质的企业，仅限从事索膜结构和和压型拱板的设计项目。"]

{"sheet":"（4）钢结构B","index":53,"n_rows":22,"n_cols":3,"rows_kept":22,"merged":[[0,0,0,2],[2,0,8,0],[2,1,4,1],[9,0,18,0],[9,1,11,1],[19,0,20,0],[21,0,21,2]],"flags":["formulas_cached_only"]}
["（4）轻型房屋钢结构工程建设项目设计规模划分表"]
["工程等级","结构类别","工程范围"]
["1级"," ","1、网架最小边跨度≥60m"]
[null,null,"2、双层网壳最小跨度≥60m"]
[null,null,"3、单层网壳最小跨度≥20m"]
[null,"      单层刚架、排架，","1、单层刚架单跨跨度≥30m，且面积不小于10000㎡；"]
[null,"多层框架等","2、排架吊车不小于20t"]
[null,null,"3、多层框架层数≤12层"]
[null,"  平面/空间桁架","单跨跨度≥24m"]
["2级","网架、网壳","1、网架最小边跨度<60m"]
[null,null,"2、双层网壳最小跨度<60m"]
[null,null,"3、单层网壳最小跨度<20m"]
[null,"    单层刚架、排架，","1、单层刚架单跨跨度<30m"]
[null,"多层框架等","2、排架吊车不小于10t"]
[null,null,"3、多层框架层数<6层"]
[null,"平面/空间桁架","单跨跨度<24m"]
[null,"冷弯薄壁型钢龙骨体系房屋","层数≤3"]
[null,"活动组合房屋","层数≤3"]
[null,"索膜结构","建筑投影面积≥100㎡"]
["不分级","索膜结构","建筑投影面积＜100㎡"]
[null,"压型拱板","单跨跨度≤30m"]
["            注：取得索膜结构和压型拱板设计资质的企业，仅限从事索膜结构和和压型拱板的设计项目。"]

{"sheet":"（5）园林景观A","index":54,"n_rows":5,"n_cols":31,"rows_kept":5,"merged":[[0,0,0,30],[1,0,2,2],[1,29,2,29],[1,30,2,30],[3,0,4,0],[3,1,4,1]],"flags":["formulas_cached_only"]}
["（5）园林景观专项设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴园林","⑵结构","⑶建筑","⑷暖通","⑸给排水","⑹电气","⑺概预算",{"$nulls":19},"总计","备   注"]
[{"$nulls":6},"公用设备〔暖通空调〕","公用设备〔给水排水〕","电气〔供配电〕"]
["专项      资质","园林    景观   工程 ","甲级",4,1,2,1,1,1,2,{"$nulls":19},12]
[null,null,"乙级",2,1,1,1,1,1,1,{"$nulls":19},8]

{"sheet":"（5）园林景观B","index":55,"n_rows":13,"n_cols":4,"rows_kept":13,"merged":[[0,0,0,3],[2,0,6,0],[2,1,6,1],[2,2,6,2],[7,0,12,0],[7,1,12,1],[7,2,12,2]],"flags":["formulas_cached_only"]}
["（5）园林景观建设项目设计规模划分表"]
["序号","工程等级","工程规模","工程范围"]
[1,"Ⅰ级","投资额＜2000万元","1、一般标准的道路绿化工程（投资规模在1000万元以内）。"]
[{"$nulls":3},"2、片林、风景林绿化工程。"]
[{"$nulls":3},"3、景观要求较高的道路绿化工程或高速路两侧绿化工程。"]
[{"$nulls":3},"4、一般标准的风景区规划方案；功能单一、技术要求简单的小型公共建筑环境；一般公共建筑工程的室外环境；相当于一星级饭店及以下标准的室外庭园设计。经济适用房的室外环境设计。"]
[{"$nulls":3},"5、城市构筑物、建筑物的艺术景观照明工程、主要街区的景观照明工程，重要绿地的景观照明工程。"]
[2,"Ⅱ级","投资额≥2000万元","1、城市重点景观道路的绿化工程，大型立交桥的绿化工程。"]
[{"$nulls":3},"2、省级和国家重点风景区规划设计工程。"]
[{"$nulls":3},"3、公园、街心花园、园林小品、屋顶花园、室内花园、城市滨水景观、环境城市道路景观带、城市广场、步行街景观设计。（注：广场设计中不含广场周边建筑及地下建筑设施）"]
[{"$nulls":3},"4、度假村、高尔夫球场的总体环境设计，高档酒店专属花园设计等景观设计工程。"]
[{"$nulls":3},"5、大型公共建筑工程室外环境设计。技术要求较复杂或有地区性意义的公共建筑工程室外环境设计。仿古建筑或高标准的古建筑、保护性建筑的室外环境设计。商业居住建筑的室外环境设计。"]
[{"$nulls":3},"6、城市构筑物、建筑物的艺术景观照明工程、主要街区的景观照明工程，重要绿地的景观照明工程。"]

{"sheet":"（6）消防设施A","index":56,"n_rows":5,"n_cols":31,"rows_kept":5,"merged":[[0,0,0,30],[1,0,2,2],[1,29,2,29],[1,30,2,30],[3,0,4,0],[3,1,4,1]],"flags":["formulas_cached_only"]}
["（6）消防设施工程专项设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴电气","⑵自动控制","⑶给排水","⑷暖通",{"$nulls":22},"总计","备   注"]
[]
["专项\n资质","消防设施工程","甲级",3,3,3,3,{"$nulls":22},12]
[null,null,"乙级",2,2,2,2,{"$nulls":22},8]

{"sheet":"（6）消防设施B","index":57,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["（6）消防设施工程建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"消防设施工程（民用建筑）","万平米","≥4万","2-4万之间","≤2万"]
[2,"消防设施工程（工业建筑）","火灾危险性","甲类乙类","丙类","丁类戊类"]

{"sheet":"（7）环境A","index":58,"n_rows":14,"n_cols":31,"rows_kept":14,"merged":[[0,0,0,30],[1,0,2,2],[1,3,1,4],[1,5,1,6],[1,8,1,9],[1,10,1,11],[1,29,2,29],[1,30,2,30],[3,0,12,0],[3,1,4,1],[5,1,6,1],[7,1,8,1],[9,1,10,1],[11,1,12,1],[11,30,12,30],[13,1,13,30]],"flags":["formulas_cached_only"]}
["（7）环境工程专项设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴环境",null,"⑵结构",null,"⑶机械","⑷土木",null,"⑸电气",null,"⑹概预算",{"$nulls":16},"总计","备   注"]
[{"$nulls":3},"环保",null,"结构〔一级〕",null,"机械","岩土",null,"电气 发电、传输"]
["\n专业      资质","水污染防治","甲级",5,2,1,1,1,null,null,1,null,1,{"$nulls":16},12]
[null,null,"乙级",3,1,1,{"$nulls":4},1,null,1,{"$nulls":16},7]
[null,"大气污染防治","甲级",5,2,1,1,1,null,null,1,null,1,{"$nulls":16},12]
[null,null,"乙级",3,1,1,null,1,null,null,1,{"$nulls":18},7]
[null,"固体废物处理处置","甲级",5,2,1,null,1,1,null,1,null,1,{"$nulls":16},12]
[null,null,"乙级",3,null,1,null,1,1,null,1,{"$nulls":18},7]
[null,"物理污染防治","甲级",5,2,1,1,1,null,null,1,null,1,{"$nulls":16},12]
[null,null,"乙级",3,1,1,null,1,null,null,1,{"$nulls":18},7]
[null,"污染   修复","甲级",5,2,1,null,null,1,1,1,null,1,{"$nulls":16},12]
[null,null,"乙级",3,1,1,null,null,1,null,1,{"$nulls":18},7]
["注： ","1.同时申请环境工程专项资质一个以上专业类别的单位，除必须满足相应专业、级别的主要专业技术人员配备要求外，还应分别提供满足所申请专业类别要求的业绩证明材料。"]

{"sheet":"（7）环境B","index":59,"n_rows":19,"n_cols":7,"rows_kept":19,"merged":[[0,0,0,6],[1,1,1,2],[2,0,4,0],[2,1,4,1],[5,0,8,0],[5,1,8,1],[9,0,15,0],[9,1,15,1],[10,2,11,2],[10,3,11,3],[16,0,17,0],[16,1,17,1]],"flags":["formulas_cached_only"]}
["（7）环境工程建设项目设计规模划分表"]
["序号","环境工程类别",null,"计算（量）单位","大型","中型","小型"]
[1,"水污染防治工程","工业废水治理","废水量：吨/日","≥5000","1000-5000","<1000"]
[null,null,"城镇污水处理","污水量：万吨/日","≥4","1-4","<1"]
[null,null,"污（废）水回用","污（废）水量：吨/日","≥10000","2000-10000","<2000"]
[2,"大气污染防治工程","工业蒸汽锅炉烟气治理","单台装机容量：蒸吨/小时","≥65","35-65","<35"]
[null,null,"发电锅炉烟气治理","单台装机容量：兆瓦","≥125","25-125","<25"]
[null,null,"工业窑炉烟气治理","废气量：万立方米/小时","≥20","6-20","<6"]
[null,null,"其他工业废气治理","废气量：万立方米/小时","＞10","3-10","<3"]
[3,"固体废物处理处置与资源化工程","一般工业固体废物处理与利用","投资额：万元","≥2000","500-2000","<500"]
[null,null,"危险废物处理处置，其中医疗废物处置","处理量：吨/日","≥20","10-20","<10"]
[{"$nulls":4},"≥10","5-10","<5"]
[null,null,"城镇生活垃圾处理"]
[null,null,"焚烧工程","处理量：吨/日","≥300","100-300","<100"]
[null,null,"卫生填埋工程","处理量：吨/日","≥800","300-800","<300"]
[null,null,"堆肥工程","处理量：吨/日","≥300","100-300","<100"]
[4,"物理污染防治工程","噪声与振动治理","投资额：万元","≥150","50-150","<50"]
[null,null,"电磁污染防治","投资额：万元","≥400","100-400","<100"]
[5,"污染修复工程","污染水体、土壤、矿山修复等工程","投资额：万元","≥3000","500-3000","<500"]

{"sheet":"（8）防腐A","index":60,"n_rows":5,"n_cols":29,"rows_kept":5,"merged":[[0,0,0,28],[1,0,2,2],[1,27,2,27],[1,28,2,28],[3,0,4,0],[3,1,4,1]],"flags":["formulas_cached_only"]}
["（8）防腐工程专项设计主要专业技术人员配备表"]
[{"$nulls":3},"⑴化学","⑵材料学","⑶机械","⑷电气",{"$nulls":20},"总计","备   注"]
[]
["专项\n资质","防腐","甲级",5,4,2,2,{"$nulls":20},13]
[null,null,"乙级",3,2,1,1,{"$nulls":20},7]

{"sheet":"（8）防腐B","index":61,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["（8）防腐工程建设项目设计规模划分表"]
["序号","建设项目","计量（算）单位","大型","中型","小型","备注"]
[1,"防腐工程（电化学保护）","万元","＞1000","500-1000","＜500"]
[2,"防腐工程（涂覆层保护）","万元","＞2000","1000-2000","＜1000"]